AT90CAN128	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
AT90CAN128	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
AT90CAN128	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
AT90CAN128	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
AT90CAN128	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
AT90CAN128	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
AT90CAN128	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
AT90CAN128	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
AT90CAN128	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; Int. Cap.; [CKSEL=0111 SUT=00]
AT90CAN128	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; Int. Cap.; [CKSEL=0111 SUT=01]
AT90CAN128	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; Int. Cap.; [CKSEL=0111 SUT=10]
AT90CAN128	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; Int. Cap.; [CKSEL=0110 SUT=00]
AT90CAN128	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; Int. Cap.; [CKSEL=0110 SUT=01]
AT90CAN128	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; Int. Cap.; [CKSEL=0110 SUT=10]
AT90CAN128	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
AT90CAN128	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
AT90CAN128	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
AT90CAN128	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
AT90CAN128	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
AT90CAN128	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
AT90CAN128	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
AT90CAN128	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
AT90CAN128	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
AT90CAN128	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
AT90CAN128	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
AT90CAN128	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
AT90CAN128	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
AT90CAN128	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
AT90CAN128	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
AT90CAN128	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
AT90CAN128	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
AT90CAN128	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
AT90CAN128	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
AT90CAN128	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
AT90CAN128	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
AT90CAN128	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
AT90CAN128	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
AT90CAN128	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
AT90CAN128	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
AT90CAN128	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
AT90CAN128	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
AT90CAN128	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
AT90CAN128	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
AT90CAN128	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
AT90CAN128	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
AT90CAN128	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
AT90CAN128	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
AT90CAN128	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
AT90CAN128	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
AT90CAN128	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
AT90CAN128	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
AT90CAN128	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
AT90CAN32	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
AT90CAN32	0x40	0x00	Clock output on PORTC7; [CKOUT=0]
AT90CAN32	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
AT90CAN32	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
AT90CAN32	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
AT90CAN32	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
AT90CAN32	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
AT90CAN32	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
AT90CAN32	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; Int. Cap.; [CKSEL=0111 SUT=00]
AT90CAN32	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; Int. Cap.; [CKSEL=0111 SUT=01]
AT90CAN32	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; Int. Cap.; [CKSEL=0111 SUT=10]
AT90CAN32	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; Int. Cap.; [CKSEL=0110 SUT=00]
AT90CAN32	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; Int. Cap.; [CKSEL=0110 SUT=01]
AT90CAN32	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; Int. Cap.; [CKSEL=0110 SUT=10]
AT90CAN32	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
AT90CAN32	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
AT90CAN32	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
AT90CAN32	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
AT90CAN32	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
AT90CAN32	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
AT90CAN32	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
AT90CAN32	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
AT90CAN32	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
AT90CAN32	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
AT90CAN32	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
AT90CAN32	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
AT90CAN32	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
AT90CAN32	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
AT90CAN32	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
AT90CAN32	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
AT90CAN32	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
AT90CAN32	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
AT90CAN32	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
AT90CAN32	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
AT90CAN32	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
AT90CAN32	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-16.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
AT90CAN32	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-16.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
AT90CAN32	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-16.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
AT90CAN32	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-16.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
AT90CAN32	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-16.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
AT90CAN64	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
AT90CAN64	0x40	0x00	Clock output on PORTC7; [CKOUT=0]
AT90CAN64	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
AT90CAN64	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
AT90CAN64	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
AT90CAN64	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
AT90CAN64	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
AT90CAN64	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
AT90CAN64	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; Int. Cap.; [CKSEL=0111 SUT=00]
AT90CAN64	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; Int. Cap.; [CKSEL=0111 SUT=01]
AT90CAN64	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; Int. Cap.; [CKSEL=0111 SUT=10]
AT90CAN64	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; Int. Cap.; [CKSEL=0110 SUT=00]
AT90CAN64	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; Int. Cap.; [CKSEL=0110 SUT=01]
AT90CAN64	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; Int. Cap.; [CKSEL=0110 SUT=10]
AT90CAN64	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
AT90CAN64	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
AT90CAN64	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
AT90CAN64	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
AT90CAN64	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
AT90CAN64	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
AT90CAN64	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
AT90CAN64	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
AT90CAN64	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
AT90CAN64	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
AT90CAN64	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
AT90CAN64	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
AT90CAN64	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
AT90CAN64	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
AT90CAN64	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
AT90CAN64	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
AT90CAN64	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
AT90CAN64	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
AT90CAN64	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
AT90CAN64	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
AT90CAN64	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
AT90CAN64	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-16.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
AT90CAN64	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-16.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
AT90CAN64	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-16.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
AT90CAN64	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-16.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
AT90CAN64	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-16.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
AT90PWM2	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
AT90PWM2	0x40	0x00	Clock output on PORTD1; [CKOUT=0]
AT90PWM2	0x3f	0x00	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0000 SUT=00]
AT90PWM2	0x3f	0x10	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0000 SUT=01]
AT90PWM2	0x3f	0x20	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0000 SUT=10]
AT90PWM2	0x3f	0x02	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0010 SUT=00]
AT90PWM2	0x3f	0x12	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0010 SUT=01]
AT90PWM2	0x3f	0x22	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0010 SUT=10]; default value
AT90PWM2	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1000 SUT=00]   
AT90PWM2	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1000 SUT=01]   
AT90PWM2	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1000 SUT=10]   
AT90PWM2	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1000 SUT=11]   
AT90PWM2	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1001 SUT=00]   
AT90PWM2	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1001 SUT=01]   
AT90PWM2	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1001 SUT=10]   
AT90PWM2	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1001 SUT=11]   
AT90PWM2	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1010 SUT=00]   
AT90PWM2	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1010 SUT=01]   
AT90PWM2	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1010 SUT=10]   
AT90PWM2	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1010 SUT=11]   
AT90PWM2	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1011 SUT=00]   
AT90PWM2	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1011 SUT=01]   
AT90PWM2	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1011 SUT=10]   
AT90PWM2	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1011 SUT=11]   
AT90PWM2	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1100 SUT=00]   
AT90PWM2	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1100 SUT=01]   
AT90PWM2	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1100 SUT=10]   
AT90PWM2	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1100 SUT=11]   
AT90PWM2	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1101 SUT=00]   
AT90PWM2	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1101 SUT=01]   
AT90PWM2	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1101 SUT=10]   
AT90PWM2	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1101 SUT=11]   
AT90PWM2	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1110 SUT=00]   
AT90PWM2	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1110 SUT=01]   
AT90PWM2	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1110 SUT=10]   
AT90PWM2	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1110 SUT=11]   
AT90PWM2	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1111 SUT=00]   
AT90PWM2	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1111 SUT=01]   
AT90PWM2	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1111 SUT=10]   
AT90PWM2	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1111 SUT=11]   
AT90PWM2	0x3f	0x03	PLL clock; Frequency 16 MHz; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms;   [CKSEL=0011 SUT=00]
AT90PWM2	0x3f	0x13	PLL clock; Frequency 16 MHz; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4.1 ms; [CKSEL=0011 SUT=01]
AT90PWM2	0x3f	0x23	PLL clock; Frequency 16 MHz; Start-up time PWRDWN/RESET: 1K CK/14 CK + 65 ms;  [CKSEL=0011 SUT=10]
AT90PWM2	0x3f	0x33	PLL clock; Frequency 16 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=0011 SUT=11]
AT90PWM2B	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
AT90PWM2B	0x40	0x00	Clock output on PORTD1; [CKOUT=0]
AT90PWM2B	0x3f	0x00	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0000 SUT=00]
AT90PWM2B	0x3f	0x10	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0000 SUT=01]
AT90PWM2B	0x3f	0x20	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0000 SUT=10]
AT90PWM2B	0x3f	0x02	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0010 SUT=00]
AT90PWM2B	0x3f	0x12	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0010 SUT=01]
AT90PWM2B	0x3f	0x22	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0010 SUT=10]; default value
AT90PWM2B	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1000 SUT=00]   
AT90PWM2B	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1000 SUT=01]   
AT90PWM2B	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1000 SUT=10]   
AT90PWM2B	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1000 SUT=11]   
AT90PWM2B	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1001 SUT=00]   
AT90PWM2B	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1001 SUT=01]   
AT90PWM2B	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1001 SUT=10]   
AT90PWM2B	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1001 SUT=11]   
AT90PWM2B	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1010 SUT=00]   
AT90PWM2B	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1010 SUT=01]   
AT90PWM2B	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1010 SUT=10]   
AT90PWM2B	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1010 SUT=11]   
AT90PWM2B	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1011 SUT=00]   
AT90PWM2B	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1011 SUT=01]   
AT90PWM2B	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1011 SUT=10]   
AT90PWM2B	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1011 SUT=11]   
AT90PWM2B	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1100 SUT=00]   
AT90PWM2B	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1100 SUT=01]   
AT90PWM2B	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1100 SUT=10]   
AT90PWM2B	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1100 SUT=11]   
AT90PWM2B	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1101 SUT=00]   
AT90PWM2B	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1101 SUT=01]   
AT90PWM2B	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1101 SUT=10]   
AT90PWM2B	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1101 SUT=11]   
AT90PWM2B	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1110 SUT=00]   
AT90PWM2B	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1110 SUT=01]   
AT90PWM2B	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1110 SUT=10]   
AT90PWM2B	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1110 SUT=11]   
AT90PWM2B	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1111 SUT=00]   
AT90PWM2B	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1111 SUT=01]   
AT90PWM2B	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1111 SUT=10]   
AT90PWM2B	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1111 SUT=11]   
AT90PWM2B	0x3f	0x03	PLL clock; Frequency 16 MHz; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms;   [CKSEL=0011 SUT=00]
AT90PWM2B	0x3f	0x13	PLL clock; Frequency 16 MHz; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4.1 ms; [CKSEL=0011 SUT=01]
AT90PWM2B	0x3f	0x23	PLL clock; Frequency 16 MHz; Start-up time PWRDWN/RESET: 1K CK/14 CK + 65 ms;  [CKSEL=0011 SUT=10]
AT90PWM2B	0x3f	0x33	PLL clock; Frequency 16 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=0011 SUT=11]
AT90PWM2B	0x3f	0x01	PLL clock /4; PLL input: Ext. Clock; Start-up time PWRDWN/RESET: 6K CK/14 CK + 0 ms;   [CKSEL=0001 SUT=00]
AT90PWM2B	0x3f	0x11	PLL clock /4; PLL input: Ext. Clock; Start-up time PWRDWN/RESET: 6K CK/14 CK + 4 ms;   [CKSEL=0001 SUT=01]
AT90PWM2B	0x3f	0x21	PLL clock /4; PLL input: Ext. Clock; Start-up time PWRDWN/RESET: 6K CK/14 CK + 64 ms;   [CKSEL=0001 SUT=10]
AT90PWM2B	0x3f	0x05	PLL clock /4; PLL input: Ext. Crystal Osc.; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms;   [CKSEL=0101 SUT=00]
AT90PWM2B	0x3f	0x15	PLL clock /4; PLL input: Ext. Crystal Osc.; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4 ms;   [CKSEL=0101 SUT=01]
AT90PWM2B	0x3f	0x25	PLL clock /4; PLL input: Ext. Crystal Osc.; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4 ms;   [CKSEL=0101 SUT=10]
AT90PWM2B	0x3f	0x35	PLL clock /4; PLL input: Ext. Crystal Osc.; Start-up time PWRDWN/RESET: 16K CK/14 CK + 64 ms;   [CKSEL=0101 SUT=11]
AT90PWM2B	0x3f	0x04	Ext. Crystal Osc.; PLL input: Ext. Crystal Osc.; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms;   [CKSEL=0100 SUT=00]
AT90PWM2B	0x3f	0x14	Ext. Crystal Osc.; PLL input: Ext. Crystal Osc.; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4 ms;   [CKSEL=0100 SUT=01]
AT90PWM2B	0x3f	0x24	Ext. Crystal Osc.; PLL input: Ext. Crystal Osc.; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4 ms;   [CKSEL=0100 SUT=10]
AT90PWM2B	0x3f	0x34	Ext. Crystal Osc.; PLL input: Ext. Crystal Osc.; Start-up time PWRDWN/RESET: 16K CK/14 CK + 64 ms;   [CKSEL=0100 SUT=11]
AT90PWM3	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
AT90PWM3	0x40	0x00	Clock output on PORTD1; [CKOUT=0]
AT90PWM3	0x3f	0x00	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0000 SUT=00]
AT90PWM3	0x3f	0x10	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0000 SUT=01]
AT90PWM3	0x3f	0x20	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0000 SUT=10]
AT90PWM3	0x3f	0x02	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0010 SUT=00]
AT90PWM3	0x3f	0x12	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0010 SUT=01]
AT90PWM3	0x3f	0x22	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0010 SUT=10]; default value
AT90PWM3	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1000 SUT=00]   
AT90PWM3	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1000 SUT=01]   
AT90PWM3	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1000 SUT=10]   
AT90PWM3	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1000 SUT=11]   
AT90PWM3	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1001 SUT=00]   
AT90PWM3	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1001 SUT=01]   
AT90PWM3	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1001 SUT=10]   
AT90PWM3	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1001 SUT=11]   
AT90PWM3	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1010 SUT=00]   
AT90PWM3	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1010 SUT=01]   
AT90PWM3	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1010 SUT=10]   
AT90PWM3	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1010 SUT=11]   
AT90PWM3	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1011 SUT=00]   
AT90PWM3	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1011 SUT=01]   
AT90PWM3	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1011 SUT=10]   
AT90PWM3	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1011 SUT=11]   
AT90PWM3	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1100 SUT=00]   
AT90PWM3	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1100 SUT=01]   
AT90PWM3	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1100 SUT=10]   
AT90PWM3	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1100 SUT=11]   
AT90PWM3	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1101 SUT=00]   
AT90PWM3	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1101 SUT=01]   
AT90PWM3	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1101 SUT=10]   
AT90PWM3	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1101 SUT=11]   
AT90PWM3	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1110 SUT=00]   
AT90PWM3	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1110 SUT=01]   
AT90PWM3	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1110 SUT=10]   
AT90PWM3	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1110 SUT=11]   
AT90PWM3	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1111 SUT=00]   
AT90PWM3	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1111 SUT=01]   
AT90PWM3	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1111 SUT=10]   
AT90PWM3	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1111 SUT=11]   
AT90PWM3	0x3f	0x03	PLL clock; Frequency 16 MHz; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms;   [CKSEL=0011 SUT=00]
AT90PWM3	0x3f	0x13	PLL clock; Frequency 16 MHz; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4.1 ms; [CKSEL=0011 SUT=01]
AT90PWM3	0x3f	0x23	PLL clock; Frequency 16 MHz; Start-up time PWRDWN/RESET: 1K CK/14 CK + 65 ms;  [CKSEL=0011 SUT=10]
AT90PWM3	0x3f	0x33	PLL clock; Frequency 16 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=0011 SUT=11]
AT90PWM3B	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
AT90PWM3B	0x40	0x00	Clock output on PORTD1; [CKOUT=0]
AT90PWM3B	0x3f	0x00	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0000 SUT=00]
AT90PWM3B	0x3f	0x10	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0000 SUT=01]
AT90PWM3B	0x3f	0x20	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0000 SUT=10]
AT90PWM3B	0x3f	0x02	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0010 SUT=00]
AT90PWM3B	0x3f	0x12	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0010 SUT=01]
AT90PWM3B	0x3f	0x22	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0010 SUT=10]; default value
AT90PWM3B	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1000 SUT=00]   
AT90PWM3B	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1000 SUT=01]   
AT90PWM3B	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1000 SUT=10]   
AT90PWM3B	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1000 SUT=11]   
AT90PWM3B	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1001 SUT=00]   
AT90PWM3B	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1001 SUT=01]   
AT90PWM3B	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1001 SUT=10]   
AT90PWM3B	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1001 SUT=11]   
AT90PWM3B	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1010 SUT=00]   
AT90PWM3B	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1010 SUT=01]   
AT90PWM3B	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1010 SUT=10]   
AT90PWM3B	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1010 SUT=11]   
AT90PWM3B	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1011 SUT=00]   
AT90PWM3B	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1011 SUT=01]   
AT90PWM3B	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1011 SUT=10]   
AT90PWM3B	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1011 SUT=11]   
AT90PWM3B	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1100 SUT=00]   
AT90PWM3B	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1100 SUT=01]   
AT90PWM3B	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1100 SUT=10]   
AT90PWM3B	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1100 SUT=11]   
AT90PWM3B	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1101 SUT=00]   
AT90PWM3B	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1101 SUT=01]   
AT90PWM3B	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1101 SUT=10]   
AT90PWM3B	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1101 SUT=11]   
AT90PWM3B	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1110 SUT=00]   
AT90PWM3B	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1110 SUT=01]   
AT90PWM3B	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1110 SUT=10]   
AT90PWM3B	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1110 SUT=11]   
AT90PWM3B	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1111 SUT=00]   
AT90PWM3B	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1111 SUT=01]   
AT90PWM3B	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1111 SUT=10]   
AT90PWM3B	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1111 SUT=11]   
AT90PWM3B	0x3f	0x03	PLL clock /4; PLL input: Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms;   [CKSEL=0011 SUT=00]
AT90PWM3B	0x3f	0x13	PLL clock /4; PLL input: Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4.1 ms; [CKSEL=0011 SUT=01]
AT90PWM3B	0x3f	0x23	PLL clock /4; PLL input: Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 1K CK/14 CK + 65 ms;  [CKSEL=0011 SUT=10]
AT90PWM3B	0x3f	0x33	PLL clock /4; PLL input: Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=0011 SUT=11]
AT90PWM3B	0x3f	0x01	PLL clock /4; PLL input: Ext. Clock; Start-up time PWRDWN/RESET: 6K CK/14 CK + 0 ms;   [CKSEL=0001 SUT=00]
AT90PWM3B	0x3f	0x11	PLL clock /4; PLL input: Ext. Clock; Start-up time PWRDWN/RESET: 6K CK/14 CK + 4 ms;   [CKSEL=0001 SUT=01]
AT90PWM3B	0x3f	0x21	PLL clock /4; PLL input: Ext. Clock; Start-up time PWRDWN/RESET: 6K CK/14 CK + 64 ms;   [CKSEL=0001 SUT=10]
AT90PWM3B	0x3f	0x05	PLL clock /4; PLL input: Ext. Crystal Osc.; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms;   [CKSEL=0101 SUT=00]
AT90PWM3B	0x3f	0x15	PLL clock /4; PLL input: Ext. Crystal Osc.; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4 ms;   [CKSEL=0101 SUT=01]
AT90PWM3B	0x3f	0x25	PLL clock /4; PLL input: Ext. Crystal Osc.; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4 ms;   [CKSEL=0101 SUT=10]
AT90PWM3B	0x3f	0x35	PLL clock /4; PLL input: Ext. Crystal Osc.; Start-up time PWRDWN/RESET: 16K CK/14 CK + 64 ms;   [CKSEL=0101 SUT=11]
AT90PWM3B	0x3f	0x04	Ext. Crystal Osc.; PLL input: Ext. Crystal Osc.; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms;   [CKSEL=0100 SUT=00]
AT90PWM3B	0x3f	0x14	Ext. Crystal Osc.; PLL input: Ext. Crystal Osc.; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4 ms;   [CKSEL=0100 SUT=01]
AT90PWM3B	0x3f	0x24	Ext. Crystal Osc.; PLL input: Ext. Crystal Osc.; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4 ms;   [CKSEL=0100 SUT=10]
AT90PWM3B	0x3f	0x34	Ext. Crystal Osc.; PLL input: Ext. Crystal Osc.; Start-up time PWRDWN/RESET: 16K CK/14 CK + 64 ms;   [CKSEL=0100 SUT=11]
AT90USB1286	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
AT90USB1286	0x40	0x00	Clock output on PORTC7; [CKOUT=0]
AT90USB1286	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
AT90USB1286	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
AT90USB1286	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
AT90USB1286	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
AT90USB1286	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
AT90USB1286	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
AT90USB1286	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; Int. Cap.; [CKSEL=0111 SUT=00]
AT90USB1286	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; Int. Cap.; [CKSEL=0111 SUT=01]
AT90USB1286	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; Int. Cap.; [CKSEL=0111 SUT=10]
AT90USB1286	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; Int. Cap.; [CKSEL=0110 SUT=00]
AT90USB1286	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; Int. Cap.; [CKSEL=0110 SUT=01]
AT90USB1286	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; Int. Cap.; [CKSEL=0110 SUT=10]
AT90USB1286	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
AT90USB1286	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
AT90USB1286	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
AT90USB1286	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
AT90USB1286	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
AT90USB1286	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
AT90USB1286	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
AT90USB1286	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
AT90USB1286	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
AT90USB1286	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
AT90USB1286	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
AT90USB1286	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
AT90USB1286	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
AT90USB1286	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
AT90USB1286	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
AT90USB1286	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
AT90USB1286	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
AT90USB1286	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
AT90USB1286	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
AT90USB1286	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
AT90USB1286	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
AT90USB1286	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
AT90USB1286	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
AT90USB1286	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
AT90USB1286	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
AT90USB1286	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
AT90USB1286	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
AT90USB1286	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
AT90USB1286	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
AT90USB1286	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
AT90USB1286	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
AT90USB1286	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
AT90USB1286	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
AT90USB1286	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
AT90USB1286	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
AT90USB1286	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
AT90USB1286	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
AT90USB1286	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
AT90USB1287	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
AT90USB1287	0x40	0x00	Clock output on PORTC7; [CKOUT=0]
AT90USB1287	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
AT90USB1287	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
AT90USB1287	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
AT90USB1287	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
AT90USB1287	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
AT90USB1287	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
AT90USB1287	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; Int. Cap.; [CKSEL=0111 SUT=00]
AT90USB1287	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; Int. Cap.; [CKSEL=0111 SUT=01]
AT90USB1287	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; Int. Cap.; [CKSEL=0111 SUT=10]
AT90USB1287	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; Int. Cap.; [CKSEL=0110 SUT=00]
AT90USB1287	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; Int. Cap.; [CKSEL=0110 SUT=01]
AT90USB1287	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; Int. Cap.; [CKSEL=0110 SUT=10]
AT90USB1287	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
AT90USB1287	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
AT90USB1287	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
AT90USB1287	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
AT90USB1287	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
AT90USB1287	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
AT90USB1287	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
AT90USB1287	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
AT90USB1287	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
AT90USB1287	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
AT90USB1287	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
AT90USB1287	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
AT90USB1287	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
AT90USB1287	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
AT90USB1287	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
AT90USB1287	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
AT90USB1287	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
AT90USB1287	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
AT90USB1287	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
AT90USB1287	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
AT90USB1287	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
AT90USB1287	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
AT90USB1287	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
AT90USB1287	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
AT90USB1287	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
AT90USB1287	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
AT90USB1287	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
AT90USB1287	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
AT90USB1287	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
AT90USB1287	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
AT90USB1287	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
AT90USB1287	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
AT90USB1287	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
AT90USB1287	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
AT90USB1287	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
AT90USB1287	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
AT90USB1287	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
AT90USB1287	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
AT90USB162	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
AT90USB162	0x40	0x00	Clock output on PORTC7; [CKOUT=0]
AT90USB162	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
AT90USB162	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
AT90USB162	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
AT90USB162	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
AT90USB162	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
AT90USB162	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
AT90USB162	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; Int. Cap.; [CKSEL=0111 SUT=00]
AT90USB162	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; Int. Cap.; [CKSEL=0111 SUT=01]
AT90USB162	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; Int. Cap.; [CKSEL=0111 SUT=10]
AT90USB162	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; Int. Cap.; [CKSEL=0110 SUT=00]
AT90USB162	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; Int. Cap.; [CKSEL=0110 SUT=01]
AT90USB162	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; Int. Cap.; [CKSEL=0110 SUT=10]
AT90USB162	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
AT90USB162	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
AT90USB162	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
AT90USB162	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
AT90USB162	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
AT90USB162	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
AT90USB162	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
AT90USB162	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
AT90USB162	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
AT90USB162	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
AT90USB162	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
AT90USB162	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
AT90USB162	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
AT90USB162	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
AT90USB162	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
AT90USB162	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
AT90USB162	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
AT90USB162	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
AT90USB162	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
AT90USB162	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
AT90USB162	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
AT90USB162	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
AT90USB162	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
AT90USB162	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
AT90USB162	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
AT90USB162	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
AT90USB162	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
AT90USB162	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
AT90USB162	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
AT90USB162	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
AT90USB162	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
AT90USB162	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
AT90USB162	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
AT90USB162	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
AT90USB162	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
AT90USB162	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
AT90USB162	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
AT90USB162	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
AT90USB646	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
AT90USB646	0x40	0x00	Clock output on PORTC7; [CKOUT=0]
AT90USB646	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
AT90USB646	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
AT90USB646	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
AT90USB646	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
AT90USB646	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
AT90USB646	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
AT90USB646	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; Int. Cap.; [CKSEL=0111 SUT=00]
AT90USB646	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; Int. Cap.; [CKSEL=0111 SUT=01]
AT90USB646	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; Int. Cap.; [CKSEL=0111 SUT=10]
AT90USB646	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; Int. Cap.; [CKSEL=0110 SUT=00]
AT90USB646	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; Int. Cap.; [CKSEL=0110 SUT=01]
AT90USB646	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; Int. Cap.; [CKSEL=0110 SUT=10]
AT90USB646	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
AT90USB646	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
AT90USB646	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
AT90USB646	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
AT90USB646	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
AT90USB646	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
AT90USB646	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
AT90USB646	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
AT90USB646	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
AT90USB646	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
AT90USB646	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
AT90USB646	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
AT90USB646	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
AT90USB646	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
AT90USB646	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
AT90USB646	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
AT90USB646	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
AT90USB646	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
AT90USB646	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
AT90USB646	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
AT90USB646	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
AT90USB646	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
AT90USB646	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
AT90USB646	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
AT90USB646	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
AT90USB646	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
AT90USB646	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
AT90USB646	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
AT90USB646	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
AT90USB646	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
AT90USB646	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
AT90USB646	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
AT90USB646	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
AT90USB646	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
AT90USB646	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
AT90USB646	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
AT90USB646	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
AT90USB646	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
AT90USB647	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
AT90USB647	0x40	0x00	Clock output on PORTC7; [CKOUT=0]
AT90USB647	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
AT90USB647	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
AT90USB647	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
AT90USB647	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
AT90USB647	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
AT90USB647	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
AT90USB647	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; Int. Cap.; [CKSEL=0111 SUT=00]
AT90USB647	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; Int. Cap.; [CKSEL=0111 SUT=01]
AT90USB647	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; Int. Cap.; [CKSEL=0111 SUT=10]
AT90USB647	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; Int. Cap.; [CKSEL=0110 SUT=00]
AT90USB647	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; Int. Cap.; [CKSEL=0110 SUT=01]
AT90USB647	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; Int. Cap.; [CKSEL=0110 SUT=10]
AT90USB647	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
AT90USB647	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
AT90USB647	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
AT90USB647	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
AT90USB647	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
AT90USB647	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
AT90USB647	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
AT90USB647	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
AT90USB647	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
AT90USB647	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
AT90USB647	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
AT90USB647	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
AT90USB647	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
AT90USB647	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
AT90USB647	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
AT90USB647	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
AT90USB647	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
AT90USB647	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
AT90USB647	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
AT90USB647	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
AT90USB647	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
AT90USB647	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
AT90USB647	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
AT90USB647	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
AT90USB647	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
AT90USB647	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
AT90USB647	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
AT90USB647	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
AT90USB647	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
AT90USB647	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
AT90USB647	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
AT90USB647	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
AT90USB647	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
AT90USB647	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
AT90USB647	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
AT90USB647	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
AT90USB647	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
AT90USB647	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega103	0x80	0x00	Brown-out detection level at VCC=4.0 V; [BODLEVEL=0]
ATmega103	0x80	0x80	Brown-out detection level at VCC=2.7 V; [BODLEVEL=1]
ATmega103	0x40	0x00	Brown-out detection enabled; [BODEN=0]
ATmega103	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega103	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4 ms; [CKSEL=0000 SUT=01]
ATmega103	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 64 ms; [CKSEL=0000 SUT=10]
ATmega103	0x3f	0x01	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0001 SUT=00]
ATmega103	0x3f	0x11	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0001 SUT=01]
ATmega103	0x3f	0x21	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0001 SUT=10]; default value
ATmega103	0x3f	0x02	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega103	0x3f	0x12	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0010 SUT=01]
ATmega103	0x3f	0x22	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0010 SUT=10]
ATmega103	0x3f	0x03	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega103	0x3f	0x13	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega103	0x3f	0x23	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega103	0x3f	0x04	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega103	0x3f	0x14	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0100 SUT=01]
ATmega103	0x3f	0x24	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0100 SUT=10]
ATmega103	0x3f	0x05	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega103	0x3f	0x15	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0101 SUT=01]
ATmega103	0x3f	0x25	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0101 SUT=10]
ATmega103	0x3f	0x35	Ext. RC Osc.         -  0.9 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0101 SUT=11]
ATmega103	0x3f	0x06	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega103	0x3f	0x16	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0110 SUT=01]
ATmega103	0x3f	0x26	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0110 SUT=10]
ATmega103	0x3f	0x36	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0110 SUT=11]
ATmega103	0x3f	0x07	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega103	0x3f	0x17	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0111 SUT=01]
ATmega103	0x3f	0x27	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0111 SUT=10]
ATmega103	0x3f	0x37	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0111 SUT=11]
ATmega103	0x3f	0x08	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=1000 SUT=00]
ATmega103	0x3f	0x18	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=1000 SUT=01]
ATmega103	0x3f	0x28	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=1000 SUT=10]
ATmega103	0x3f	0x38	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=1000 SUT=11]
ATmega103	0x3f	0x09	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4 ms; [CKSEL=1001 SUT=00]
ATmega103	0x3f	0x19	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 64 ms; [CKSEL=1001 SUT=01]
ATmega103	0x3f	0x29	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 64 ms; [CKSEL=1001 SUT=10]
ATmega103	0x3f	0x0a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1010 SUT=00]
ATmega103	0x3f	0x1a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1010 SUT=01]
ATmega103	0x3f	0x2a	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega103	0x3f	0x3a	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1010 SUT=11]
ATmega103	0x3f	0x0b	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1011 SUT=00]
ATmega103	0x3f	0x1b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega103	0x3f	0x2b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1011 SUT=10]
ATmega103	0x3f	0x3b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1011 SUT=11]
ATmega103	0x3f	0x0c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1100 SUT=00]
ATmega103	0x3f	0x1c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1100 SUT=01]
ATmega103	0x3f	0x2c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega103	0x3f	0x3c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1100 SUT=11]
ATmega103	0x3f	0x0d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1101 SUT=00]
ATmega103	0x3f	0x1d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega103	0x3f	0x2d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1101 SUT=10]
ATmega103	0x3f	0x3d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1101 SUT=11]
ATmega103	0x3f	0x0e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1110 SUT=00]
ATmega103	0x3f	0x1e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1110 SUT=01]
ATmega103	0x3f	0x2e	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega103	0x3f	0x3e	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1110 SUT=11]
ATmega103	0x3f	0x0f	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1111 SUT=00]
ATmega103	0x3f	0x1f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega103	0x3f	0x2f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1111 SUT=10]
ATmega103	0x3f	0x3f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1111 SUT=11]
ATmega128	0x80	0x00	Brown-out detection level at VCC=4.0 V; [BODLEVEL=0]
ATmega128	0x80	0x80	Brown-out detection level at VCC=2.7 V; [BODLEVEL=1]
ATmega128	0x40	0x00	Brown-out detection enabled; [BODEN=0]
ATmega128	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega128	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4 ms; [CKSEL=0000 SUT=01]
ATmega128	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 64 ms; [CKSEL=0000 SUT=10]
ATmega128	0x3f	0x01	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0001 SUT=00]
ATmega128	0x3f	0x11	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0001 SUT=01]
ATmega128	0x3f	0x21	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0001 SUT=10]; default value
ATmega128	0x3f	0x02	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega128	0x3f	0x12	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0010 SUT=01]
ATmega128	0x3f	0x22	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0010 SUT=10]
ATmega128	0x3f	0x03	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega128	0x3f	0x13	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega128	0x3f	0x23	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega128	0x3f	0x04	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega128	0x3f	0x14	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0100 SUT=01]
ATmega128	0x3f	0x24	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0100 SUT=10]
ATmega128	0x3f	0x05	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega128	0x3f	0x15	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0101 SUT=01]
ATmega128	0x3f	0x25	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0101 SUT=10]
ATmega128	0x3f	0x35	Ext. RC Osc.         -  0.9 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0101 SUT=11]
ATmega128	0x3f	0x06	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega128	0x3f	0x16	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0110 SUT=01]
ATmega128	0x3f	0x26	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0110 SUT=10]
ATmega128	0x3f	0x36	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0110 SUT=11]
ATmega128	0x3f	0x07	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega128	0x3f	0x17	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0111 SUT=01]
ATmega128	0x3f	0x27	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0111 SUT=10]
ATmega128	0x3f	0x37	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0111 SUT=11]
ATmega128	0x3f	0x08	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=1000 SUT=00]
ATmega128	0x3f	0x18	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=1000 SUT=01]
ATmega128	0x3f	0x28	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=1000 SUT=10]
ATmega128	0x3f	0x38	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=1000 SUT=11]
ATmega128	0x3f	0x09	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4 ms; [CKSEL=1001 SUT=00]
ATmega128	0x3f	0x19	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 64 ms; [CKSEL=1001 SUT=01]
ATmega128	0x3f	0x29	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 64 ms; [CKSEL=1001 SUT=10]
ATmega128	0x3f	0x0a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1010 SUT=00]
ATmega128	0x3f	0x1a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1010 SUT=01]
ATmega128	0x3f	0x2a	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega128	0x3f	0x3a	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1010 SUT=11]
ATmega128	0x3f	0x0b	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1011 SUT=00]
ATmega128	0x3f	0x1b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega128	0x3f	0x2b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1011 SUT=10]
ATmega128	0x3f	0x3b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1011 SUT=11]
ATmega128	0x3f	0x0c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1100 SUT=00]
ATmega128	0x3f	0x1c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1100 SUT=01]
ATmega128	0x3f	0x2c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega128	0x3f	0x3c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1100 SUT=11]
ATmega128	0x3f	0x0d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1101 SUT=00]
ATmega128	0x3f	0x1d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega128	0x3f	0x2d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1101 SUT=10]
ATmega128	0x3f	0x3d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1101 SUT=11]
ATmega128	0x3f	0x0e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1110 SUT=00]
ATmega128	0x3f	0x1e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1110 SUT=01]
ATmega128	0x3f	0x2e	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega128	0x3f	0x3e	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1110 SUT=11]
ATmega128	0x3f	0x0f	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1111 SUT=00]
ATmega128	0x3f	0x1f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega128	0x3f	0x2f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1111 SUT=10]
ATmega128	0x3f	0x3f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1111 SUT=11]
ATmega1280	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega1280	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
ATmega1280	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega1280	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega1280	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega1280	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega1280	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega1280	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega1280	0x3f	0x03	Int. 128kHz RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega1280	0x3f	0x13	Int. 128kHz RC Osc.; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega1280	0x3f	0x23	Int. 128kHz RC Osc.; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega1280	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega1280	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
ATmega1280	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
ATmega1280	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega1280	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
ATmega1280	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
ATmega1280	0x3f	0x06	Full Swing Oscillator; Start-up time: 258 CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=00]
ATmega1280	0x3f	0x16	Full Swing Oscillator; Start-up time: 258 CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0110 SUT=01]
ATmega1280	0x3f	0x26	Full Swing Oscillator; Start-up time: 1K CK + 0 ms; Ceramic res.; BOD enable; [CKSEL=0110 SUT=10]
ATmega1280	0x3f	0x36	Full Swing Oscillator; Start-up time: 1K CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=11]
ATmega1280	0x3f	0x07	Full Swing Oscillator; Start-up time: 1K CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0111 SUT=00]
ATmega1280	0x3f	0x17	Full Swing Oscillator; Start-up time: 16K CK + 0 ms; Crystal Osc.; BOD enabled; [CKSEL=0111 SUT=01]
ATmega1280	0x3f	0x27	Full Swing Oscillator; Start-up time: 16K CK + 4.1 ms; Crystal Osc.; fast rising power; [CKSEL=0111 SUT=10]
ATmega1280	0x3f	0x37	Full Swing Oscillator; Start-up time: 16K CK + 65 ms; Crystal Osc.; slowly rising power; [CKSEL=0111 SUT=11]
ATmega1280	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega1280	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega1280	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega1280	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega1280	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega1280	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega1280	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega1280	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega1280	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega1280	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega1280	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega1280	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega1280	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega1280	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega1280	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega1280	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega1280	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega1280	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega1280	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega1280	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega1280	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega1280	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega1280	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega1280	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega1280	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega1280	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega1280	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega1280	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega1280	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega1280	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega1280	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega1280	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega1281	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega1281	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
ATmega1281	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega1281	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega1281	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega1281	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega1281	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega1281	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega1281	0x3f	0x03	Int. 128kHz RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega1281	0x3f	0x13	Int. 128kHz RC Osc.; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega1281	0x3f	0x23	Int. 128kHz RC Osc.; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega1281	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega1281	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
ATmega1281	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
ATmega1281	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega1281	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
ATmega1281	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
ATmega1281	0x3f	0x06	Full Swing Oscillator; Start-up time: 258 CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=00]
ATmega1281	0x3f	0x16	Full Swing Oscillator; Start-up time: 258 CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0110 SUT=01]
ATmega1281	0x3f	0x26	Full Swing Oscillator; Start-up time: 1K CK + 0 ms; Ceramic res.; BOD enable; [CKSEL=0110 SUT=10]
ATmega1281	0x3f	0x36	Full Swing Oscillator; Start-up time: 1K CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=11]
ATmega1281	0x3f	0x07	Full Swing Oscillator; Start-up time: 1K CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0111 SUT=00]
ATmega1281	0x3f	0x17	Full Swing Oscillator; Start-up time: 16K CK + 0 ms; Crystal Osc.; BOD enabled; [CKSEL=0111 SUT=01]
ATmega1281	0x3f	0x27	Full Swing Oscillator; Start-up time: 16K CK + 4.1 ms; Crystal Osc.; fast rising power; [CKSEL=0111 SUT=10]
ATmega1281	0x3f	0x37	Full Swing Oscillator; Start-up time: 16K CK + 65 ms; Crystal Osc.; slowly rising power; [CKSEL=0111 SUT=11]
ATmega1281	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega1281	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega1281	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega1281	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega1281	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega1281	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega1281	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega1281	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega1281	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega1281	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega1281	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega1281	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega1281	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega1281	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega1281	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega1281	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega1281	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega1281	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega1281	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega1281	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega1281	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega1281	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega1281	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega1281	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega1281	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega1281	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega1281	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega1281	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega1281	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega1281	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega1281	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega1281	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega16	0x80	0x00	Brown-out detection level at VCC=4.0 V; [BODLEVEL=0]
ATmega16	0x80	0x80	Brown-out detection level at VCC=2.7 V; [BODLEVEL=1]
ATmega16	0x40	0x00	Brown-out detection enabled; [BODEN=0]
ATmega16	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega16	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4 ms; [CKSEL=0000 SUT=01]
ATmega16	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 64 ms; [CKSEL=0000 SUT=10]
ATmega16	0x3f	0x01	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0001 SUT=00]
ATmega16	0x3f	0x11	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0001 SUT=01]
ATmega16	0x3f	0x21	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0001 SUT=10]; default value
ATmega16	0x3f	0x02	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega16	0x3f	0x12	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0010 SUT=01]
ATmega16	0x3f	0x22	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0010 SUT=10]
ATmega16	0x3f	0x03	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega16	0x3f	0x13	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega16	0x3f	0x23	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega16	0x3f	0x04	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega16	0x3f	0x14	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0100 SUT=01]
ATmega16	0x3f	0x24	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0100 SUT=10]
ATmega16	0x3f	0x05	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega16	0x3f	0x15	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0101 SUT=01]
ATmega16	0x3f	0x25	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0101 SUT=10]
ATmega16	0x3f	0x35	Ext. RC Osc.         -  0.9 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0101 SUT=11]
ATmega16	0x3f	0x06	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega16	0x3f	0x16	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0110 SUT=01]
ATmega16	0x3f	0x26	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0110 SUT=10]
ATmega16	0x3f	0x36	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0110 SUT=11]
ATmega16	0x3f	0x07	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega16	0x3f	0x17	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0111 SUT=01]
ATmega16	0x3f	0x27	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0111 SUT=10]
ATmega16	0x3f	0x37	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0111 SUT=11]
ATmega16	0x3f	0x08	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=1000 SUT=00]
ATmega16	0x3f	0x18	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=1000 SUT=01]
ATmega16	0x3f	0x28	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=1000 SUT=10]
ATmega16	0x3f	0x38	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=1000 SUT=11]
ATmega16	0x3f	0x09	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4 ms; [CKSEL=1001 SUT=00]
ATmega16	0x3f	0x19	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 64 ms; [CKSEL=1001 SUT=01]
ATmega16	0x3f	0x29	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 64 ms; [CKSEL=1001 SUT=10]
ATmega16	0x3f	0x0a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1010 SUT=00]
ATmega16	0x3f	0x1a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1010 SUT=01]
ATmega16	0x3f	0x2a	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega16	0x3f	0x3a	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1010 SUT=11]
ATmega16	0x3f	0x0b	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1011 SUT=00]
ATmega16	0x3f	0x1b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega16	0x3f	0x2b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1011 SUT=10]
ATmega16	0x3f	0x3b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1011 SUT=11]
ATmega16	0x3f	0x0c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1100 SUT=00]
ATmega16	0x3f	0x1c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1100 SUT=01]
ATmega16	0x3f	0x2c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega16	0x3f	0x3c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1100 SUT=11]
ATmega16	0x3f	0x0d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1101 SUT=00]
ATmega16	0x3f	0x1d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega16	0x3f	0x2d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1101 SUT=10]
ATmega16	0x3f	0x3d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1101 SUT=11]
ATmega16	0x3f	0x0e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1110 SUT=00]
ATmega16	0x3f	0x1e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1110 SUT=01]
ATmega16	0x3f	0x2e	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega16	0x3f	0x3e	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1110 SUT=11]
ATmega16	0x3f	0x0f	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1111 SUT=00]
ATmega16	0x3f	0x1f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega16	0x3f	0x2f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1111 SUT=10]
ATmega16	0x3f	0x3f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1111 SUT=11]
ATmega161	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega161	0x40	0x00	Clock output on PORTB0; [CKOUT=0]
ATmega161	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega161	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega161	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega161	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega161	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega161	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega161	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; Int. Cap.; [CKSEL=0111 SUT=00]
ATmega161	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; Int. Cap.; [CKSEL=0111 SUT=01]
ATmega161	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; Int. Cap.; [CKSEL=0111 SUT=10]
ATmega161	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; Int. Cap.; [CKSEL=0110 SUT=00]
ATmega161	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; Int. Cap.; [CKSEL=0110 SUT=01]
ATmega161	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; Int. Cap.; [CKSEL=0110 SUT=10]
ATmega161	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega161	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
ATmega161	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
ATmega161	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega161	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
ATmega161	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
ATmega161	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega161	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega161	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega161	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega161	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega161	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega161	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega161	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega161	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega161	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega161	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega161	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega161	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega161	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega161	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega161	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega161	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega161	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega161	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega161	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega161	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega161	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega161	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega161	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega161	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega161	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega161	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega161	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega161	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega161	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega161	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega161	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega162	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega162	0x40	0x00	Clock output on PORTB0; [CKOUT=0]
ATmega162	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega162	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega162	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega162	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega162	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega162	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega162	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; Int. Cap.; [CKSEL=0111 SUT=00]
ATmega162	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; Int. Cap.; [CKSEL=0111 SUT=01]
ATmega162	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; Int. Cap.; [CKSEL=0111 SUT=10]
ATmega162	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; Int. Cap.; [CKSEL=0110 SUT=00]
ATmega162	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; Int. Cap.; [CKSEL=0110 SUT=01]
ATmega162	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; Int. Cap.; [CKSEL=0110 SUT=10]
ATmega162	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega162	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
ATmega162	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
ATmega162	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega162	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
ATmega162	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
ATmega162	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega162	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega162	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega162	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega162	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega162	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega162	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega162	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega162	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega162	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega162	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega162	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega162	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega162	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega162	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega162	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega162	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega162	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega162	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega162	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega162	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega162	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega162	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega162	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega162	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega162	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega162	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega162	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega162	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega162	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega162	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega162	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega163	0x80	0x00	Brown-out detection level at VCC=4.0 V
ATmega163	0x80	0x80	Brown-out detection level at VCC=2.7 V
ATmega163	0x40	0x00	Brown-out detection enabled
ATmega163	0x20	0x00	Serial program downloading (SPI) enabled
ATmega163	0x0f	0x00	CKSEL=0000 External Clock fast rising power
ATmega163	0x0f	0x01	CKSEL=0001 External Clock BOD enabled
ATmega163	0x0f	0x02	CKSEL=0010 Internal RC Ocsillator slowly rising power ; default value
ATmega163	0x0f	0x03	CKSEL=0011 Internal RC Ocsillator fast rising power
ATmega163	0x0f	0x04	CKSEL=0100 Internal RC Oscillator BOD enabled
ATmega163	0x0f	0x05	CKSEL=0101 External RC Oscillator slowly rising power
ATmega163	0x0f	0x06	CKSEL=0110 External RC Oscillator fast rising power
ATmega163	0x0f	0x07	CKSEL=0111 External RC Oscillator BOD enabled
ATmega163	0x0f	0x08	CKSEL=1000 External Low-Frequency Crystal
ATmega163	0x0f	0x09	CKSEL=1001 External Low-Frequency Crystal
ATmega163	0x0f	0x0a	CKSEL=1010 Crystal Oscillator slowly rising power
ATmega163	0x0f	0x0b	CKSEL=1011 Crystal Oscillator fast rising power
ATmega163	0x0f	0x0c	CKSEL=1100 Crystal Oscillator BOD enabled
ATmega163	0x0f	0x0d	CKSEL=1101 Ceramic Resonator/External Clock slowly rising power
ATmega163	0x0f	0x0e	CKSEL=1110 Ceramic Resonator fast rising power
ATmega163	0x0f	0x0f	CKSEL=1111 Ceramic Resonator BOD enabled
ATmega164P	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega164P	0x40	0x00	Clock output on PORTB1; [CKOUT=0]
ATmega164P	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega164P	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega164P	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega164P	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega164P	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega164P	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega164P	0x3f	0x03	Int. 128kHz RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega164P	0x3f	0x13	Int. 128kHz RC Osc.; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega164P	0x3f	0x23	Int. 128kHz RC Osc.; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega164P	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega164P	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
ATmega164P	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
ATmega164P	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega164P	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
ATmega164P	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
ATmega164P	0x3f	0x06	Full Swing Oscillator; Start-up time: 258 CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=00]
ATmega164P	0x3f	0x16	Full Swing Oscillator; Start-up time: 258 CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0110 SUT=01]
ATmega164P	0x3f	0x26	Full Swing Oscillator; Start-up time: 1K CK + 0 ms; Ceramic res.; BOD enable; [CKSEL=0110 SUT=10]
ATmega164P	0x3f	0x36	Full Swing Oscillator; Start-up time: 1K CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=11]
ATmega164P	0x3f	0x07	Full Swing Oscillator; Start-up time: 1K CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0111 SUT=00]
ATmega164P	0x3f	0x17	Full Swing Oscillator; Start-up time: 16K CK + 0 ms; Crystal Osc.; BOD enabled; [CKSEL=0111 SUT=01]
ATmega164P	0x3f	0x27	Full Swing Oscillator; Start-up time: 16K CK + 4.1 ms; Crystal Osc.; fast rising power; [CKSEL=0111 SUT=10]
ATmega164P	0x3f	0x37	Full Swing Oscillator; Start-up time: 16K CK + 65 ms; Crystal Osc.; slowly rising power; [CKSEL=0111 SUT=11]
ATmega164P	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega164P	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega164P	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega164P	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega164P	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega164P	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega164P	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega164P	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega164P	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega164P	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega164P	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega164P	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega164P	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega164P	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega164P	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega164P	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega164P	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega164P	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega164P	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega164P	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega164P	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega164P	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega164P	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega164P	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega164P	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega164P	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega164P	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega164P	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega164P	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega164P	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega164P	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega164P	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega168	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega168	0x40	0x00	Clock output on PORTB0; [CKOUT=0]
ATmega168	0x3f	0x00	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0000 SUT=00]
ATmega168	0x3f	0x10	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega168	0x3f	0x20	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0000 SUT=10]
ATmega168	0x3f	0x02	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0010 SUT=00]
ATmega168	0x3f	0x12	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega168	0x3f	0x22	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0010 SUT=10]; default value
ATmega168	0x3f	0x03	Int. RC Osc. 128kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0011 SUT=00]
ATmega168	0x3f	0x13	Int. RC Osc. 128kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0011 SUT=01]
ATmega168	0x3f	0x23	Int. RC Osc. 128kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0011 SUT=10]
ATmega168	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms;   [CKSEL=0100 SUT=00] 
ATmega168	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4.1 ms; [CKSEL=0100 SUT=01] 
ATmega168	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 65 ms;  [CKSEL=0100 SUT=10] 
ATmega168	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32K CK/14 CK + 0 ms;   [CKSEL=0101 SUT=00] 
ATmega168	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32K CK/14 CK + 4.1 ms; [CKSEL=0101 SUT=01] 
ATmega168	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32K CK/14 CK + 65 ms;  [CKSEL=0101 SUT=10] 
ATmega168	0x3f	0x06	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms;[CKSEL=0110 SUT=00] 
ATmega168	0x3f	0x16	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms; [CKSEL=0110 SUT=01] 
ATmega168	0x3f	0x26	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;  [CKSEL=0110 SUT=10] 
ATmega168	0x3f	0x36	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms;[CKSEL=0110 SUT=11] 
ATmega168	0x3f	0x07	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms; [CKSEL=0111 SUT=00] 
ATmega168	0x3f	0x17	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;  [CKSEL=0111 SUT=01] 
ATmega168	0x3f	0x27	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms;[CKSEL=0111 SUT=10] 
ATmega168	0x3f	0x37	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms; [CKSEL=0111 SUT=11] 
ATmega168	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1000 SUT=00]   
ATmega168	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1000 SUT=01]   
ATmega168	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1000 SUT=10]   
ATmega168	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1000 SUT=11]   
ATmega168	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1001 SUT=00]   
ATmega168	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1001 SUT=01]   
ATmega168	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1001 SUT=10]   
ATmega168	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1001 SUT=11]   
ATmega168	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1010 SUT=00]   
ATmega168	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1010 SUT=01]   
ATmega168	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1010 SUT=10]   
ATmega168	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1010 SUT=11]   
ATmega168	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1011 SUT=00]   
ATmega168	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1011 SUT=01]   
ATmega168	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1011 SUT=10]   
ATmega168	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1011 SUT=11]   
ATmega168	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1100 SUT=00]   
ATmega168	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1100 SUT=01]   
ATmega168	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1100 SUT=10]   
ATmega168	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1100 SUT=11]   
ATmega168	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1101 SUT=00]   
ATmega168	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1101 SUT=01]   
ATmega168	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1101 SUT=10]   
ATmega168	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1101 SUT=11]   
ATmega168	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1110 SUT=00]   
ATmega168	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1110 SUT=01]   
ATmega168	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1110 SUT=10]   
ATmega168	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1110 SUT=11]   
ATmega168	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1111 SUT=00]   
ATmega168	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1111 SUT=01]   
ATmega168	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1111 SUT=10]   
ATmega168	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1111 SUT=11]   
ATmega169	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega169	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
ATmega169	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega169	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega169	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega169	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega169	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega169	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega169	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega169	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0111 SUT=01]
ATmega169	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0111 SUT=10]
ATmega169	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega169	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0110 SUT=01]
ATmega169	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0110 SUT=10]
ATmega169	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega169	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega169	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega169	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega169	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega169	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega169	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega169	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega169	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega169	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega169	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega169	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega169	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega169	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega169	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega169	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega169	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega169	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega169	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega169	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega169	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega169	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega169	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega169	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega169	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega169	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega169	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega169	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega169	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega169	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega169	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega169	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega2560	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega2560	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
ATmega2560	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega2560	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega2560	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega2560	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega2560	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega2560	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega2560	0x3f	0x03	Int. 128kHz RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega2560	0x3f	0x13	Int. 128kHz RC Osc.; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega2560	0x3f	0x23	Int. 128kHz RC Osc.; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega2560	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega2560	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
ATmega2560	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
ATmega2560	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega2560	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
ATmega2560	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
ATmega2560	0x3f	0x06	Full Swing Oscillator; Start-up time: 258 CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=00]
ATmega2560	0x3f	0x16	Full Swing Oscillator; Start-up time: 258 CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0110 SUT=01]
ATmega2560	0x3f	0x26	Full Swing Oscillator; Start-up time: 1K CK + 0 ms; Ceramic res.; BOD enable; [CKSEL=0110 SUT=10]
ATmega2560	0x3f	0x36	Full Swing Oscillator; Start-up time: 1K CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=11]
ATmega2560	0x3f	0x07	Full Swing Oscillator; Start-up time: 1K CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0111 SUT=00]
ATmega2560	0x3f	0x17	Full Swing Oscillator; Start-up time: 16K CK + 0 ms; Crystal Osc.; BOD enabled; [CKSEL=0111 SUT=01]
ATmega2560	0x3f	0x27	Full Swing Oscillator; Start-up time: 16K CK + 4.1 ms; Crystal Osc.; fast rising power; [CKSEL=0111 SUT=10]
ATmega2560	0x3f	0x37	Full Swing Oscillator; Start-up time: 16K CK + 65 ms; Crystal Osc.; slowly rising power; [CKSEL=0111 SUT=11]
ATmega2560	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega2560	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega2560	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega2560	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega2560	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega2560	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega2560	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega2560	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega2560	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega2560	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega2560	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega2560	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega2560	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega2560	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega2560	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega2560	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega2560	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega2560	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega2560	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega2560	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega2560	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega2560	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega2560	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega2560	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega2560	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega2560	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega2560	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega2560	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega2560	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega2560	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega2560	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega2560	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega2561	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega2561	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
ATmega2561	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega2561	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega2561	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega2561	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega2561	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega2561	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega2561	0x3f	0x03	Int. 128kHz RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega2561	0x3f	0x13	Int. 128kHz RC Osc.; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega2561	0x3f	0x23	Int. 128kHz RC Osc.; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega2561	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega2561	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
ATmega2561	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
ATmega2561	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega2561	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
ATmega2561	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
ATmega2561	0x3f	0x06	Full Swing Oscillator; Start-up time: 258 CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=00]
ATmega2561	0x3f	0x16	Full Swing Oscillator; Start-up time: 258 CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0110 SUT=01]
ATmega2561	0x3f	0x26	Full Swing Oscillator; Start-up time: 1K CK + 0 ms; Ceramic res.; BOD enable; [CKSEL=0110 SUT=10]
ATmega2561	0x3f	0x36	Full Swing Oscillator; Start-up time: 1K CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=11]
ATmega2561	0x3f	0x07	Full Swing Oscillator; Start-up time: 1K CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0111 SUT=00]
ATmega2561	0x3f	0x17	Full Swing Oscillator; Start-up time: 16K CK + 0 ms; Crystal Osc.; BOD enabled; [CKSEL=0111 SUT=01]
ATmega2561	0x3f	0x27	Full Swing Oscillator; Start-up time: 16K CK + 4.1 ms; Crystal Osc.; fast rising power; [CKSEL=0111 SUT=10]
ATmega2561	0x3f	0x37	Full Swing Oscillator; Start-up time: 16K CK + 65 ms; Crystal Osc.; slowly rising power; [CKSEL=0111 SUT=11]
ATmega2561	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega2561	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega2561	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega2561	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega2561	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega2561	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega2561	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega2561	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega2561	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega2561	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega2561	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega2561	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega2561	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega2561	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega2561	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega2561	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega2561	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega2561	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega2561	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega2561	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega2561	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega2561	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega2561	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega2561	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega2561	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega2561	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega2561	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega2561	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega2561	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega2561	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega2561	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega2561	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega32	0x80	0x00	Brown-out detection level at VCC=4.0 V; [BODLEVEL=0]
ATmega32	0x80	0x80	Brown-out detection level at VCC=2.7 V; [BODLEVEL=1]
ATmega32	0x40	0x00	Brown-out detection enabled; [BODEN=0]
ATmega32	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega32	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4 ms; [CKSEL=0000 SUT=01]
ATmega32	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 64 ms; [CKSEL=0000 SUT=10]
ATmega32	0x3f	0x01	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0001 SUT=00]
ATmega32	0x3f	0x11	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0001 SUT=01]
ATmega32	0x3f	0x21	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0001 SUT=10]; default value
ATmega32	0x3f	0x02	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega32	0x3f	0x12	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0010 SUT=01]
ATmega32	0x3f	0x22	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0010 SUT=10]
ATmega32	0x3f	0x03	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega32	0x3f	0x13	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega32	0x3f	0x23	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega32	0x3f	0x04	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega32	0x3f	0x14	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0100 SUT=01]
ATmega32	0x3f	0x24	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0100 SUT=10]
ATmega32	0x3f	0x05	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega32	0x3f	0x15	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0101 SUT=01]
ATmega32	0x3f	0x25	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0101 SUT=10]
ATmega32	0x3f	0x35	Ext. RC Osc.         -  0.9 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0101 SUT=11]
ATmega32	0x3f	0x06	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega32	0x3f	0x16	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0110 SUT=01]
ATmega32	0x3f	0x26	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0110 SUT=10]
ATmega32	0x3f	0x36	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0110 SUT=11]
ATmega32	0x3f	0x07	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega32	0x3f	0x17	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0111 SUT=01]
ATmega32	0x3f	0x27	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0111 SUT=10]
ATmega32	0x3f	0x37	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0111 SUT=11]
ATmega32	0x3f	0x08	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=1000 SUT=00]
ATmega32	0x3f	0x18	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=1000 SUT=01]
ATmega32	0x3f	0x28	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=1000 SUT=10]
ATmega32	0x3f	0x38	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=1000 SUT=11]
ATmega32	0x3f	0x09	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4 ms; [CKSEL=1001 SUT=00]
ATmega32	0x3f	0x19	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 64 ms; [CKSEL=1001 SUT=01]
ATmega32	0x3f	0x29	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 64 ms; [CKSEL=1001 SUT=10]
ATmega32	0x3f	0x0a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1010 SUT=00]
ATmega32	0x3f	0x1a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1010 SUT=01]
ATmega32	0x3f	0x2a	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega32	0x3f	0x3a	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1010 SUT=11]
ATmega32	0x3f	0x0b	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1011 SUT=00]
ATmega32	0x3f	0x1b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega32	0x3f	0x2b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1011 SUT=10]
ATmega32	0x3f	0x3b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1011 SUT=11]
ATmega32	0x3f	0x0c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1100 SUT=00]
ATmega32	0x3f	0x1c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1100 SUT=01]
ATmega32	0x3f	0x2c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega32	0x3f	0x3c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1100 SUT=11]
ATmega32	0x3f	0x0d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1101 SUT=00]
ATmega32	0x3f	0x1d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega32	0x3f	0x2d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1101 SUT=10]
ATmega32	0x3f	0x3d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1101 SUT=11]
ATmega32	0x3f	0x0e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1110 SUT=00]
ATmega32	0x3f	0x1e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1110 SUT=01]
ATmega32	0x3f	0x2e	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega32	0x3f	0x3e	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1110 SUT=11]
ATmega32	0x3f	0x0f	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1111 SUT=00]
ATmega32	0x3f	0x1f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega32	0x3f	0x2f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1111 SUT=10]
ATmega32	0x3f	0x3f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1111 SUT=11]
ATmega324P	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega324P	0x40	0x00	Clock output on PORTB1; [CKOUT=0]
ATmega324P	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega324P	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega324P	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega324P	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega324P	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega324P	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega324P	0x3f	0x03	Int. 128kHz RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega324P	0x3f	0x13	Int. 128kHz RC Osc.; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega324P	0x3f	0x23	Int. 128kHz RC Osc.; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega324P	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega324P	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
ATmega324P	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
ATmega324P	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega324P	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
ATmega324P	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
ATmega324P	0x3f	0x06	Full Swing Oscillator; Start-up time: 258 CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=00]
ATmega324P	0x3f	0x16	Full Swing Oscillator; Start-up time: 258 CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0110 SUT=01]
ATmega324P	0x3f	0x26	Full Swing Oscillator; Start-up time: 1K CK + 0 ms; Ceramic res.; BOD enable; [CKSEL=0110 SUT=10]
ATmega324P	0x3f	0x36	Full Swing Oscillator; Start-up time: 1K CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=11]
ATmega324P	0x3f	0x07	Full Swing Oscillator; Start-up time: 1K CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0111 SUT=00]
ATmega324P	0x3f	0x17	Full Swing Oscillator; Start-up time: 16K CK + 0 ms; Crystal Osc.; BOD enabled; [CKSEL=0111 SUT=01]
ATmega324P	0x3f	0x27	Full Swing Oscillator; Start-up time: 16K CK + 4.1 ms; Crystal Osc.; fast rising power; [CKSEL=0111 SUT=10]
ATmega324P	0x3f	0x37	Full Swing Oscillator; Start-up time: 16K CK + 65 ms; Crystal Osc.; slowly rising power; [CKSEL=0111 SUT=11]
ATmega324P	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega324P	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega324P	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega324P	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega324P	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega324P	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega324P	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega324P	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega324P	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega324P	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega324P	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega324P	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega324P	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega324P	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega324P	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega324P	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega324P	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega324P	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega324P	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega324P	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega324P	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega324P	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega324P	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega324P	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega324P	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega324P	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega324P	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega324P	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega324P	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega324P	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega324P	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega324P	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega325	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega325	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
ATmega325	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega325	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega325	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega325	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega325	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega325	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega325	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega325	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0111 SUT=01]
ATmega325	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0111 SUT=10]
ATmega325	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega325	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0110 SUT=01]
ATmega325	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0110 SUT=10]
ATmega325	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega325	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega325	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega325	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega325	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega325	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega325	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega325	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega325	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega325	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega325	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega325	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega325	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega325	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega325	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega325	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega325	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega325	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega325	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega325	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega325	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega325	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega325	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega325	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega325	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega325	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega325	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega325	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega325	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega325	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega325	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega325	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega3250	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega3250	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
ATmega3250	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega3250	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega3250	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega3250	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega3250	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega3250	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega3250	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega3250	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0111 SUT=01]
ATmega3250	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0111 SUT=10]
ATmega3250	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega3250	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0110 SUT=01]
ATmega3250	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0110 SUT=10]
ATmega3250	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega3250	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega3250	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega3250	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega3250	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega3250	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega3250	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega3250	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega3250	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega3250	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega3250	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega3250	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega3250	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega3250	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega3250	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega3250	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega3250	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega3250	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega3250	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega3250	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega3250	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega3250	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega3250	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega3250	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega3250	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega3250	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega3250	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega3250	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega3250	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega3250	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega3250	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega3250	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega329	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega329	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
ATmega329	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega329	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega329	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega329	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega329	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega329	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega329	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega329	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0111 SUT=01]
ATmega329	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0111 SUT=10]
ATmega329	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega329	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0110 SUT=01]
ATmega329	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0110 SUT=10]
ATmega329	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega329	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega329	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega329	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega329	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega329	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega329	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega329	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega329	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega329	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega329	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega329	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega329	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega329	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega329	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega329	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega329	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega329	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega329	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega329	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega329	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega329	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega329	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega329	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega329	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega329	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega329	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega329	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega329	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega329	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega329	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega329	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega3290	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega3290	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
ATmega3290	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega3290	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega3290	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega3290	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega3290	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega3290	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega3290	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega3290	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0111 SUT=01]
ATmega3290	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0111 SUT=10]
ATmega3290	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega3290	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0110 SUT=01]
ATmega3290	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0110 SUT=10]
ATmega3290	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega3290	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega3290	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega3290	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega3290	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega3290	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega3290	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega3290	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega3290	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega3290	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega3290	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega3290	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega3290	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega3290	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega3290	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega3290	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega3290	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega3290	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega3290	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega3290	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega3290	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega3290	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega3290	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega3290	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega3290	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega3290	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega3290	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega3290	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega3290	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega3290	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega3290	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega3290	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega3290P	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega3290P	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
ATmega3290P	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega3290P	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega3290P	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega3290P	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega3290P	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega3290P	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega3290P	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega3290P	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0111 SUT=01]
ATmega3290P	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0111 SUT=10]
ATmega3290P	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega3290P	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0110 SUT=01]
ATmega3290P	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0110 SUT=10]
ATmega3290P	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega3290P	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega3290P	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega3290P	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega3290P	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega3290P	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega3290P	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega3290P	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega3290P	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega3290P	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega3290P	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega3290P	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega3290P	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega3290P	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega3290P	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega3290P	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega3290P	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega3290P	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega3290P	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega3290P	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega3290P	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega3290P	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega3290P	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega3290P	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega3290P	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega3290P	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega3290P	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega3290P	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega3290P	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega3290P	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega3290P	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega3290P	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega329P	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega329P	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
ATmega329P	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega329P	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega329P	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega329P	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega329P	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega329P	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega329P	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega329P	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0111 SUT=01]
ATmega329P	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0111 SUT=10]
ATmega329P	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega329P	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0110 SUT=01]
ATmega329P	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0110 SUT=10]
ATmega329P	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega329P	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega329P	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega329P	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega329P	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega329P	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega329P	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega329P	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega329P	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega329P	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega329P	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega329P	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega329P	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega329P	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega329P	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega329P	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega329P	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega329P	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega329P	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega329P	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega329P	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega329P	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega329P	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega329P	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega329P	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega329P	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega329P	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega329P	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega329P	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega329P	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega329P	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega329P	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega48	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega48	0x40	0x00	Clock output on PORTB0; [CKOUT=0]
ATmega48	0x3f	0x00	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0000 SUT=00]
ATmega48	0x3f	0x10	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega48	0x3f	0x20	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0000 SUT=10]
ATmega48	0x3f	0x02	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0010 SUT=00]
ATmega48	0x3f	0x12	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega48	0x3f	0x22	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0010 SUT=10]; default value
ATmega48	0x3f	0x03	Int. RC Osc. 128kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0011 SUT=00]
ATmega48	0x3f	0x13	Int. RC Osc. 128kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0011 SUT=01]
ATmega48	0x3f	0x23	Int. RC Osc. 128kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0011 SUT=10]
ATmega48	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms;   [CKSEL=0100 SUT=00] 
ATmega48	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4.1 ms; [CKSEL=0100 SUT=01] 
ATmega48	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 65 ms;  [CKSEL=0100 SUT=10] 
ATmega48	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32K CK/14 CK + 0 ms;   [CKSEL=0101 SUT=00] 
ATmega48	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32K CK/14 CK + 4.1 ms; [CKSEL=0101 SUT=01] 
ATmega48	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32K CK/14 CK + 65 ms;  [CKSEL=0101 SUT=10] 
ATmega48	0x3f	0x06	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms;[CKSEL=0110 SUT=00] 
ATmega48	0x3f	0x16	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms; [CKSEL=0110 SUT=01] 
ATmega48	0x3f	0x26	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;  [CKSEL=0110 SUT=10] 
ATmega48	0x3f	0x36	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms;[CKSEL=0110 SUT=11] 
ATmega48	0x3f	0x07	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms; [CKSEL=0111 SUT=00] 
ATmega48	0x3f	0x17	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;  [CKSEL=0111 SUT=01] 
ATmega48	0x3f	0x27	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms;[CKSEL=0111 SUT=10] 
ATmega48	0x3f	0x37	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms; [CKSEL=0111 SUT=11] 
ATmega48	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1000 SUT=00]   
ATmega48	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1000 SUT=01]   
ATmega48	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1000 SUT=10]   
ATmega48	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1000 SUT=11]   
ATmega48	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1001 SUT=00]   
ATmega48	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1001 SUT=01]   
ATmega48	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1001 SUT=10]   
ATmega48	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1001 SUT=11]   
ATmega48	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1010 SUT=00]   
ATmega48	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1010 SUT=01]   
ATmega48	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1010 SUT=10]   
ATmega48	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1010 SUT=11]   
ATmega48	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1011 SUT=00]   
ATmega48	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1011 SUT=01]   
ATmega48	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1011 SUT=10]   
ATmega48	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1011 SUT=11]   
ATmega48	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1100 SUT=00]   
ATmega48	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1100 SUT=01]   
ATmega48	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1100 SUT=10]   
ATmega48	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1100 SUT=11]   
ATmega48	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1101 SUT=00]   
ATmega48	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1101 SUT=01]   
ATmega48	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1101 SUT=10]   
ATmega48	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1101 SUT=11]   
ATmega48	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1110 SUT=00]   
ATmega48	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1110 SUT=01]   
ATmega48	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1110 SUT=10]   
ATmega48	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1110 SUT=11]   
ATmega48	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1111 SUT=00]   
ATmega48	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1111 SUT=01]   
ATmega48	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1111 SUT=10]   
ATmega48	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1111 SUT=11]   
ATmega64	0x80	0x00	Brown-out detection level at VCC=4.0 V; [BODLEVEL=0]
ATmega64	0x80	0x80	Brown-out detection level at VCC=2.7 V; [BODLEVEL=1]
ATmega64	0x40	0x00	Brown-out detection enabled; [BODEN=0]
ATmega64	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega64	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4 ms; [CKSEL=0000 SUT=01]
ATmega64	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 64 ms; [CKSEL=0000 SUT=10]
ATmega64	0x3f	0x01	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0001 SUT=00]
ATmega64	0x3f	0x11	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0001 SUT=01]
ATmega64	0x3f	0x21	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0001 SUT=10]; default value
ATmega64	0x3f	0x02	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega64	0x3f	0x12	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0010 SUT=01]
ATmega64	0x3f	0x22	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0010 SUT=10]
ATmega64	0x3f	0x03	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega64	0x3f	0x13	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega64	0x3f	0x23	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega64	0x3f	0x04	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega64	0x3f	0x14	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0100 SUT=01]
ATmega64	0x3f	0x24	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0100 SUT=10]
ATmega64	0x3f	0x05	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega64	0x3f	0x15	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0101 SUT=01]
ATmega64	0x3f	0x25	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0101 SUT=10]
ATmega64	0x3f	0x35	Ext. RC Osc.         -  0.9 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0101 SUT=11]
ATmega64	0x3f	0x06	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega64	0x3f	0x16	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0110 SUT=01]
ATmega64	0x3f	0x26	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0110 SUT=10]
ATmega64	0x3f	0x36	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0110 SUT=11]
ATmega64	0x3f	0x07	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega64	0x3f	0x17	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0111 SUT=01]
ATmega64	0x3f	0x27	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0111 SUT=10]
ATmega64	0x3f	0x37	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0111 SUT=11]
ATmega64	0x3f	0x08	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=1000 SUT=00]
ATmega64	0x3f	0x18	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=1000 SUT=01]
ATmega64	0x3f	0x28	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=1000 SUT=10]
ATmega64	0x3f	0x38	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=1000 SUT=11]
ATmega64	0x3f	0x09	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4 ms; [CKSEL=1001 SUT=00]
ATmega64	0x3f	0x19	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 64 ms; [CKSEL=1001 SUT=01]
ATmega64	0x3f	0x29	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 64 ms; [CKSEL=1001 SUT=10]
ATmega64	0x3f	0x0a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1010 SUT=00]
ATmega64	0x3f	0x1a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1010 SUT=01]
ATmega64	0x3f	0x2a	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega64	0x3f	0x3a	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1010 SUT=11]
ATmega64	0x3f	0x0b	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1011 SUT=00]
ATmega64	0x3f	0x1b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega64	0x3f	0x2b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1011 SUT=10]
ATmega64	0x3f	0x3b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1011 SUT=11]
ATmega64	0x3f	0x0c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1100 SUT=00]
ATmega64	0x3f	0x1c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1100 SUT=01]
ATmega64	0x3f	0x2c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega64	0x3f	0x3c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1100 SUT=11]
ATmega64	0x3f	0x0d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1101 SUT=00]
ATmega64	0x3f	0x1d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega64	0x3f	0x2d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1101 SUT=10]
ATmega64	0x3f	0x3d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1101 SUT=11]
ATmega64	0x3f	0x0e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1110 SUT=00]
ATmega64	0x3f	0x1e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1110 SUT=01]
ATmega64	0x3f	0x2e	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega64	0x3f	0x3e	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1110 SUT=11]
ATmega64	0x3f	0x0f	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1111 SUT=00]
ATmega64	0x3f	0x1f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega64	0x3f	0x2f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1111 SUT=10]
ATmega64	0x3f	0x3f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1111 SUT=11]
ATmega640	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega640	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
ATmega640	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega640	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega640	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega640	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega640	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega640	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega640	0x3f	0x03	Int. 128kHz RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega640	0x3f	0x13	Int. 128kHz RC Osc.; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega640	0x3f	0x23	Int. 128kHz RC Osc.; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega640	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega640	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
ATmega640	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
ATmega640	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega640	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
ATmega640	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
ATmega640	0x3f	0x06	Full Swing Oscillator; Start-up time: 258 CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=00]
ATmega640	0x3f	0x16	Full Swing Oscillator; Start-up time: 258 CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0110 SUT=01]
ATmega640	0x3f	0x26	Full Swing Oscillator; Start-up time: 1K CK + 0 ms; Ceramic res.; BOD enable; [CKSEL=0110 SUT=10]
ATmega640	0x3f	0x36	Full Swing Oscillator; Start-up time: 1K CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=11]
ATmega640	0x3f	0x07	Full Swing Oscillator; Start-up time: 1K CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0111 SUT=00]
ATmega640	0x3f	0x17	Full Swing Oscillator; Start-up time: 16K CK + 0 ms; Crystal Osc.; BOD enabled; [CKSEL=0111 SUT=01]
ATmega640	0x3f	0x27	Full Swing Oscillator; Start-up time: 16K CK + 4.1 ms; Crystal Osc.; fast rising power; [CKSEL=0111 SUT=10]
ATmega640	0x3f	0x37	Full Swing Oscillator; Start-up time: 16K CK + 65 ms; Crystal Osc.; slowly rising power; [CKSEL=0111 SUT=11]
ATmega640	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega640	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega640	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega640	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega640	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega640	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega640	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega640	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega640	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega640	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega640	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega640	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega640	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega640	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega640	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega640	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega640	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega640	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega640	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega640	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega640	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega640	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega640	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega640	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega640	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega640	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega640	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega640	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega640	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega640	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega640	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega640	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega644	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega644	0x40	0x00	Clock output on PORTB1; [CKOUT=0]
ATmega644	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega644	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega644	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega644	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega644	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega644	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega644	0x3f	0x03	Int. 128kHz RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega644	0x3f	0x13	Int. 128kHz RC Osc.; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega644	0x3f	0x23	Int. 128kHz RC Osc.; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega644	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega644	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
ATmega644	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
ATmega644	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega644	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
ATmega644	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
ATmega644	0x3f	0x06	Full Swing Oscillator; Start-up time: 258 CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=00]
ATmega644	0x3f	0x16	Full Swing Oscillator; Start-up time: 258 CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0110 SUT=01]
ATmega644	0x3f	0x26	Full Swing Oscillator; Start-up time: 1K CK + 0 ms; Ceramic res.; BOD enable; [CKSEL=0110 SUT=10]
ATmega644	0x3f	0x36	Full Swing Oscillator; Start-up time: 1K CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=11]
ATmega644	0x3f	0x07	Full Swing Oscillator; Start-up time: 1K CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0111 SUT=00]
ATmega644	0x3f	0x17	Full Swing Oscillator; Start-up time: 16K CK + 0 ms; Crystal Osc.; BOD enabled; [CKSEL=0111 SUT=01]
ATmega644	0x3f	0x27	Full Swing Oscillator; Start-up time: 16K CK + 4.1 ms; Crystal Osc.; fast rising power; [CKSEL=0111 SUT=10]
ATmega644	0x3f	0x37	Full Swing Oscillator; Start-up time: 16K CK + 65 ms; Crystal Osc.; slowly rising power; [CKSEL=0111 SUT=11]
ATmega644	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega644	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega644	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega644	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega644	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega644	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega644	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega644	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega644	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega644	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega644	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega644	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega644	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega644	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega644	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega644	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega644	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega644	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega644	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega644	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega644	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega644	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega644	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega644	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega644	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega644	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega644	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega644	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega644	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega644	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega644	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega644	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega644P	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega644P	0x40	0x00	Clock output on PORTB1; [CKOUT=0]
ATmega644P	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega644P	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega644P	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega644P	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega644P	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega644P	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega644P	0x3f	0x03	Int. 128kHz RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega644P	0x3f	0x13	Int. 128kHz RC Osc.; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega644P	0x3f	0x23	Int. 128kHz RC Osc.; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega644P	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega644P	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0100 SUT=01]
ATmega644P	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0100 SUT=10]
ATmega644P	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega644P	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0101 SUT=01]
ATmega644P	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0101 SUT=10]
ATmega644P	0x3f	0x06	Full Swing Oscillator; Start-up time: 258 CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=00]
ATmega644P	0x3f	0x16	Full Swing Oscillator; Start-up time: 258 CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0110 SUT=01]
ATmega644P	0x3f	0x26	Full Swing Oscillator; Start-up time: 1K CK + 0 ms; Ceramic res.; BOD enable; [CKSEL=0110 SUT=10]
ATmega644P	0x3f	0x36	Full Swing Oscillator; Start-up time: 1K CK + 4.1 ms; Ceramic res.; fast rising power; [CKSEL=0110 SUT=11]
ATmega644P	0x3f	0x07	Full Swing Oscillator; Start-up time: 1K CK + 65 ms; Ceramic res.; slowly rising power; [CKSEL=0111 SUT=00]
ATmega644P	0x3f	0x17	Full Swing Oscillator; Start-up time: 16K CK + 0 ms; Crystal Osc.; BOD enabled; [CKSEL=0111 SUT=01]
ATmega644P	0x3f	0x27	Full Swing Oscillator; Start-up time: 16K CK + 4.1 ms; Crystal Osc.; fast rising power; [CKSEL=0111 SUT=10]
ATmega644P	0x3f	0x37	Full Swing Oscillator; Start-up time: 16K CK + 65 ms; Crystal Osc.; slowly rising power; [CKSEL=0111 SUT=11]
ATmega644P	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega644P	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega644P	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega644P	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega644P	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega644P	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega644P	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega644P	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega644P	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega644P	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega644P	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega644P	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega644P	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega644P	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega644P	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega644P	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega644P	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega644P	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega644P	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega644P	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega644P	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega644P	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega644P	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega644P	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega644P	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega644P	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega644P	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega644P	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega644P	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega644P	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega644P	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega644P	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega645	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega645	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
ATmega645	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega645	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega645	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega645	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega645	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega645	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega645	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega645	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0111 SUT=01]
ATmega645	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0111 SUT=10]
ATmega645	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega645	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0110 SUT=01]
ATmega645	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0110 SUT=10]
ATmega645	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega645	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega645	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega645	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega645	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega645	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega645	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega645	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega645	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega645	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega645	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega645	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega645	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega645	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega645	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega645	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega645	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega645	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega645	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega645	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega645	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega645	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega645	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega645	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega645	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega645	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega645	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega645	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega645	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega645	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega645	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega645	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega6450	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega6450	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
ATmega6450	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega6450	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega6450	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega6450	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega6450	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega6450	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega6450	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega6450	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0111 SUT=01]
ATmega6450	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0111 SUT=10]
ATmega6450	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega6450	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0110 SUT=01]
ATmega6450	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0110 SUT=10]
ATmega6450	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega6450	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega6450	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega6450	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega6450	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega6450	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega6450	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega6450	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega6450	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega6450	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega6450	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega6450	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega6450	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega6450	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega6450	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega6450	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega6450	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega6450	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega6450	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega6450	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega6450	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega6450	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega6450	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega6450	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega6450	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega6450	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega6450	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega6450	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega6450	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega6450	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega6450	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega6450	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega649	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega649	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
ATmega649	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega649	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega649	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega649	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega649	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega649	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega649	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega649	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0111 SUT=01]
ATmega649	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0111 SUT=10]
ATmega649	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega649	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0110 SUT=01]
ATmega649	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0110 SUT=10]
ATmega649	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega649	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega649	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega649	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega649	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega649	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega649	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega649	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega649	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega649	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega649	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega649	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega649	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega649	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega649	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega649	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega649	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega649	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega649	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega649	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega649	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega649	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega649	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega649	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega649	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega649	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega649	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega649	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega649	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega649	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega649	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega649	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega6490	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega6490	0x40	0x00	Clock output on PORTE7; [CKOUT=0]
ATmega6490	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega6490	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega6490	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 65 ms; [CKSEL=0000 SUT=10]
ATmega6490	0x3f	0x02	Int. RC Osc.; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega6490	0x3f	0x12	Int. RC Osc.; Start-up time: 6 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega6490	0x3f	0x22	Int. RC Osc.; Start-up time: 6 CK + 65 ms; [CKSEL=0010 SUT=10]
ATmega6490	0x3f	0x07	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega6490	0x3f	0x17	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 4.1 ms; [CKSEL=0111 SUT=01]
ATmega6490	0x3f	0x27	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 65 ms; [CKSEL=0111 SUT=10]
ATmega6490	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega6490	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4.1 ms; [CKSEL=0110 SUT=01]
ATmega6490	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 65 ms; [CKSEL=0110 SUT=10]
ATmega6490	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATmega6490	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1000 SUT=01]
ATmega6490	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1000 SUT=10]
ATmega6490	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATmega6490	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1001 SUT=00]
ATmega6490	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1001 SUT=01]
ATmega6490	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATmega6490	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1001 SUT=11]
ATmega6490	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATmega6490	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1010 SUT=01]
ATmega6490	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega6490	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATmega6490	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1011 SUT=00]
ATmega6490	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega6490	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATmega6490	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1011 SUT=11]
ATmega6490	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATmega6490	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1100 SUT=01]
ATmega6490	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega6490	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATmega6490	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1101 SUT=00]
ATmega6490	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega6490	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATmega6490	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1101 SUT=11]
ATmega6490	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATmega6490	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 258 CK + 65 ms; [CKSEL=1110 SUT=01]
ATmega6490	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega6490	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATmega6490	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 1K CK + 65 ms; [CKSEL=1111 SUT=00]
ATmega6490	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega6490	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATmega6490	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 16K CK + 65 ms; [CKSEL=1111 SUT=11]
ATmega8	0x80	0x00	Brown-out detection level at VCC=4.0 V; [BODLEVEL=0]
ATmega8	0x80	0x80	Brown-out detection level at VCC=2.7 V; [BODLEVEL=1]
ATmega8	0x40	0x00	Brown-out detection enabled; [BODEN=0]
ATmega8	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega8	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4 ms; [CKSEL=0000 SUT=01]
ATmega8	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 64 ms; [CKSEL=0000 SUT=10]
ATmega8	0x3f	0x01	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0001 SUT=00]
ATmega8	0x3f	0x11	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0001 SUT=01]
ATmega8	0x3f	0x21	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0001 SUT=10]; default value
ATmega8	0x3f	0x02	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega8	0x3f	0x12	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0010 SUT=01]
ATmega8	0x3f	0x22	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0010 SUT=10]
ATmega8	0x3f	0x03	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega8	0x3f	0x13	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega8	0x3f	0x23	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega8	0x3f	0x04	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega8	0x3f	0x14	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0100 SUT=01]
ATmega8	0x3f	0x24	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0100 SUT=10]
ATmega8	0x3f	0x05	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega8	0x3f	0x15	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0101 SUT=01]
ATmega8	0x3f	0x25	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0101 SUT=10]
ATmega8	0x3f	0x35	Ext. RC Osc.         -  0.9 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0101 SUT=11]
ATmega8	0x3f	0x06	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega8	0x3f	0x16	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0110 SUT=01]
ATmega8	0x3f	0x26	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0110 SUT=10]
ATmega8	0x3f	0x36	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0110 SUT=11]
ATmega8	0x3f	0x07	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega8	0x3f	0x17	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0111 SUT=01]
ATmega8	0x3f	0x27	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0111 SUT=10]
ATmega8	0x3f	0x37	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0111 SUT=11]
ATmega8	0x3f	0x08	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=1000 SUT=00]
ATmega8	0x3f	0x18	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=1000 SUT=01]
ATmega8	0x3f	0x28	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=1000 SUT=10]
ATmega8	0x3f	0x38	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=1000 SUT=11]
ATmega8	0x3f	0x09	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4 ms; [CKSEL=1001 SUT=00]
ATmega8	0x3f	0x19	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 64 ms; [CKSEL=1001 SUT=01]
ATmega8	0x3f	0x29	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 64 ms; [CKSEL=1001 SUT=10]
ATmega8	0x3f	0x0a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1010 SUT=00]
ATmega8	0x3f	0x1a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1010 SUT=01]
ATmega8	0x3f	0x2a	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega8	0x3f	0x3a	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1010 SUT=11]
ATmega8	0x3f	0x0b	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1011 SUT=00]
ATmega8	0x3f	0x1b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega8	0x3f	0x2b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1011 SUT=10]
ATmega8	0x3f	0x3b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1011 SUT=11]
ATmega8	0x3f	0x0c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1100 SUT=00]
ATmega8	0x3f	0x1c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1100 SUT=01]
ATmega8	0x3f	0x2c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega8	0x3f	0x3c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1100 SUT=11]
ATmega8	0x3f	0x0d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1101 SUT=00]
ATmega8	0x3f	0x1d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega8	0x3f	0x2d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1101 SUT=10]
ATmega8	0x3f	0x3d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1101 SUT=11]
ATmega8	0x3f	0x0e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1110 SUT=00]
ATmega8	0x3f	0x1e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1110 SUT=01]
ATmega8	0x3f	0x2e	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega8	0x3f	0x3e	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1110 SUT=11]
ATmega8	0x3f	0x0f	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1111 SUT=00]
ATmega8	0x3f	0x1f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega8	0x3f	0x2f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1111 SUT=10]
ATmega8	0x3f	0x3f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1111 SUT=11]
ATmega8515	0x80	0x00	Brown-out detection level at VCC=4.0 V; [BODLEVEL=0]
ATmega8515	0x80	0x80	Brown-out detection level at VCC=2.7 V; [BODLEVEL=1]
ATmega8515	0x40	0x00	Brown-out detection enabled; [BODEN=0]
ATmega8515	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega8515	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4 ms; [CKSEL=0000 SUT=01]
ATmega8515	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 64 ms; [CKSEL=0000 SUT=10]
ATmega8515	0x3f	0x01	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0001 SUT=00]
ATmega8515	0x3f	0x11	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0001 SUT=01]
ATmega8515	0x3f	0x21	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0001 SUT=10]; default value
ATmega8515	0x3f	0x02	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega8515	0x3f	0x12	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0010 SUT=01]
ATmega8515	0x3f	0x22	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0010 SUT=10]
ATmega8515	0x3f	0x03	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega8515	0x3f	0x13	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega8515	0x3f	0x23	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega8515	0x3f	0x04	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega8515	0x3f	0x14	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0100 SUT=01]
ATmega8515	0x3f	0x24	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0100 SUT=10]
ATmega8515	0x3f	0x05	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega8515	0x3f	0x15	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0101 SUT=01]
ATmega8515	0x3f	0x25	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0101 SUT=10]
ATmega8515	0x3f	0x35	Ext. RC Osc.         -  0.9 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0101 SUT=11]
ATmega8515	0x3f	0x06	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega8515	0x3f	0x16	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0110 SUT=01]
ATmega8515	0x3f	0x26	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0110 SUT=10]
ATmega8515	0x3f	0x36	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0110 SUT=11]
ATmega8515	0x3f	0x07	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega8515	0x3f	0x17	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0111 SUT=01]
ATmega8515	0x3f	0x27	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0111 SUT=10]
ATmega8515	0x3f	0x37	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0111 SUT=11]
ATmega8515	0x3f	0x08	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=1000 SUT=00]
ATmega8515	0x3f	0x18	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=1000 SUT=01]
ATmega8515	0x3f	0x28	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=1000 SUT=10]
ATmega8515	0x3f	0x38	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=1000 SUT=11]
ATmega8515	0x3f	0x09	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4 ms; [CKSEL=1001 SUT=00]
ATmega8515	0x3f	0x19	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 64 ms; [CKSEL=1001 SUT=01]
ATmega8515	0x3f	0x29	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 64 ms; [CKSEL=1001 SUT=10]
ATmega8515	0x3f	0x0a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1010 SUT=00]
ATmega8515	0x3f	0x1a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1010 SUT=01]
ATmega8515	0x3f	0x2a	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega8515	0x3f	0x3a	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1010 SUT=11]
ATmega8515	0x3f	0x0b	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1011 SUT=00]
ATmega8515	0x3f	0x1b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega8515	0x3f	0x2b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1011 SUT=10]
ATmega8515	0x3f	0x3b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1011 SUT=11]
ATmega8515	0x3f	0x0c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1100 SUT=00]
ATmega8515	0x3f	0x1c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1100 SUT=01]
ATmega8515	0x3f	0x2c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega8515	0x3f	0x3c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1100 SUT=11]
ATmega8515	0x3f	0x0d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1101 SUT=00]
ATmega8515	0x3f	0x1d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega8515	0x3f	0x2d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1101 SUT=10]
ATmega8515	0x3f	0x3d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1101 SUT=11]
ATmega8515	0x3f	0x0e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1110 SUT=00]
ATmega8515	0x3f	0x1e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1110 SUT=01]
ATmega8515	0x3f	0x2e	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega8515	0x3f	0x3e	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1110 SUT=11]
ATmega8515	0x3f	0x0f	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1111 SUT=00]
ATmega8515	0x3f	0x1f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega8515	0x3f	0x2f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1111 SUT=10]
ATmega8515	0x3f	0x3f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 64 ms;[CKSEL=1111 SUT=11]
ATmega8535	0x80	0x00	Brown-out detection level at VCC=4.0 V; [BODLEVEL=0]
ATmega8535	0x80	0x80	Brown-out detection level at VCC=2.7 V; [BODLEVEL=1]
ATmega8535	0x40	0x00	Brown-out detection enabled; [BODEN=0]
ATmega8535	0x3f	0x00	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATmega8535	0x3f	0x10	Ext. Clock; Start-up time: 6 CK + 4 ms; [CKSEL=0000 SUT=01]
ATmega8535	0x3f	0x20	Ext. Clock; Start-up time: 6 CK + 64 ms; [CKSEL=0000 SUT=10]
ATmega8535	0x3f	0x01	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0001 SUT=00]
ATmega8535	0x3f	0x11	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0001 SUT=01]
ATmega8535	0x3f	0x21	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0001 SUT=10]; default value
ATmega8535	0x3f	0x02	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATmega8535	0x3f	0x12	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0010 SUT=01]
ATmega8535	0x3f	0x22	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0010 SUT=10]
ATmega8535	0x3f	0x03	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATmega8535	0x3f	0x13	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATmega8535	0x3f	0x23	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATmega8535	0x3f	0x04	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0100 SUT=00]
ATmega8535	0x3f	0x14	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0100 SUT=01]
ATmega8535	0x3f	0x24	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0100 SUT=10]
ATmega8535	0x3f	0x05	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0101 SUT=00]
ATmega8535	0x3f	0x15	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0101 SUT=01]
ATmega8535	0x3f	0x25	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0101 SUT=10]
ATmega8535	0x3f	0x35	Ext. RC Osc.         -  0.9 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0101 SUT=11]
ATmega8535	0x3f	0x06	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0110 SUT=00]
ATmega8535	0x3f	0x16	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0110 SUT=01]
ATmega8535	0x3f	0x26	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0110 SUT=10]
ATmega8535	0x3f	0x36	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0110 SUT=11]
ATmega8535	0x3f	0x07	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0111 SUT=00]
ATmega8535	0x3f	0x17	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0111 SUT=01]
ATmega8535	0x3f	0x27	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0111 SUT=10]
ATmega8535	0x3f	0x37	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0111 SUT=11]
ATmega8535	0x3f	0x08	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=1000 SUT=00]
ATmega8535	0x3f	0x18	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=1000 SUT=01]
ATmega8535	0x3f	0x28	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=1000 SUT=10]
ATmega8535	0x3f	0x38	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=1000 SUT=11]
ATmega8535	0x3f	0x09	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4 ms; [CKSEL=1001 SUT=00]
ATmega8535	0x3f	0x19	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 64 ms; [CKSEL=1001 SUT=01]
ATmega8535	0x3f	0x29	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 64 ms; [CKSEL=1001 SUT=10]
ATmega8535	0x3f	0x0a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1010 SUT=00]
ATmega8535	0x3f	0x1a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1010 SUT=01]
ATmega8535	0x3f	0x2a	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATmega8535	0x3f	0x3a	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1010 SUT=11]
ATmega8535	0x3f	0x0b	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1011 SUT=00]
ATmega8535	0x3f	0x1b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATmega8535	0x3f	0x2b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1011 SUT=10]
ATmega8535	0x3f	0x3b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1011 SUT=11]
ATmega8535	0x3f	0x0c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1100 SUT=00]
ATmega8535	0x3f	0x1c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1100 SUT=01]
ATmega8535	0x3f	0x2c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATmega8535	0x3f	0x3c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1100 SUT=11]
ATmega8535	0x3f	0x0d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1101 SUT=00]
ATmega8535	0x3f	0x1d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATmega8535	0x3f	0x2d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1101 SUT=10]
ATmega8535	0x3f	0x3d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1101 SUT=11]
ATmega8535	0x3f	0x0e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1110 SUT=00]
ATmega8535	0x3f	0x1e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1110 SUT=01]
ATmega8535	0x3f	0x2e	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATmega8535	0x3f	0x3e	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1110 SUT=11]
ATmega8535	0x3f	0x0f	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1111 SUT=00]
ATmega8535	0x3f	0x1f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATmega8535	0x3f	0x2f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1111 SUT=10]
ATmega8535	0x3f	0x3f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 64 ms;[CKSEL=1111 SUT=11]
ATmega88	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATmega88	0x40	0x00	Clock output on PORTB0; [CKOUT=0]
ATmega88	0x3f	0x00	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0000 SUT=00]
ATmega88	0x3f	0x10	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATmega88	0x3f	0x20	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0000 SUT=10]
ATmega88	0x3f	0x02	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0010 SUT=00]
ATmega88	0x3f	0x12	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATmega88	0x3f	0x22	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0010 SUT=10]; default value
ATmega88	0x3f	0x03	Int. RC Osc. 128kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0011 SUT=00]
ATmega88	0x3f	0x13	Int. RC Osc. 128kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0011 SUT=01]
ATmega88	0x3f	0x23	Int. RC Osc. 128kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0011 SUT=10]
ATmega88	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms;   [CKSEL=0100 SUT=00] 
ATmega88	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4.1 ms; [CKSEL=0100 SUT=01] 
ATmega88	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 65 ms;  [CKSEL=0100 SUT=10] 
ATmega88	0x3f	0x05	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32K CK/14 CK + 0 ms;   [CKSEL=0101 SUT=00] 
ATmega88	0x3f	0x15	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32K CK/14 CK + 4.1 ms; [CKSEL=0101 SUT=01] 
ATmega88	0x3f	0x25	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32K CK/14 CK + 65 ms;  [CKSEL=0101 SUT=10] 
ATmega88	0x3f	0x06	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms;[CKSEL=0110 SUT=00] 
ATmega88	0x3f	0x16	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms; [CKSEL=0110 SUT=01] 
ATmega88	0x3f	0x26	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;  [CKSEL=0110 SUT=10] 
ATmega88	0x3f	0x36	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms;[CKSEL=0110 SUT=11] 
ATmega88	0x3f	0x07	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms; [CKSEL=0111 SUT=00] 
ATmega88	0x3f	0x17	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;  [CKSEL=0111 SUT=01] 
ATmega88	0x3f	0x27	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms;[CKSEL=0111 SUT=10] 
ATmega88	0x3f	0x37	Ext. Full-swing Crystal; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms; [CKSEL=0111 SUT=11] 
ATmega88	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1000 SUT=00]   
ATmega88	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1000 SUT=01]   
ATmega88	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1000 SUT=10]   
ATmega88	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1000 SUT=11]   
ATmega88	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1001 SUT=00]   
ATmega88	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1001 SUT=01]   
ATmega88	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1001 SUT=10]   
ATmega88	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1001 SUT=11]   
ATmega88	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1010 SUT=00]   
ATmega88	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1010 SUT=01]   
ATmega88	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1010 SUT=10]   
ATmega88	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1010 SUT=11]   
ATmega88	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1011 SUT=00]   
ATmega88	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1011 SUT=01]   
ATmega88	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1011 SUT=10]   
ATmega88	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1011 SUT=11]   
ATmega88	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1100 SUT=00]   
ATmega88	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1100 SUT=01]   
ATmega88	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1100 SUT=10]   
ATmega88	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1100 SUT=11]   
ATmega88	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1101 SUT=00]   
ATmega88	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1101 SUT=01]   
ATmega88	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1101 SUT=10]   
ATmega88	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1101 SUT=11]   
ATmega88	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1110 SUT=00]   
ATmega88	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1110 SUT=01]   
ATmega88	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1110 SUT=10]   
ATmega88	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1110 SUT=11]   
ATmega88	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1111 SUT=00]   
ATmega88	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1111 SUT=01]   
ATmega88	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1111 SUT=10]   
ATmega88	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1111 SUT=11]   
ATtiny11	0x10	0x00	Short start-up time selected
ATtiny11	0x08	0x00	External reset function of PB5 disabled
ATtiny11	0x07	0x07	CKSEL=111 External Crystal / Ceramic Resonator
ATtiny11	0x07	0x06	CKSEL=110 External Low-frequency Crystal
ATtiny11	0x07	0x05	CKSEL=101 External RC Oscillator
ATtiny11	0x07	0x04	CKSEL=100 Internal RC Oscillator
ATtiny11	0x07	0x00	CKSEL=000 External Clock
ATtiny12	0x80	0x80	Brown-out detection level at VCC=1.8 V
ATtiny12	0x80	0x00	Brown-out detection level at VCC=2.7 V
ATtiny12	0x40	0x00	Brown-out detection enabled
ATtiny12	0x20	0x00	Serial program downloading (SPI) enabled
ATtiny12	0x10	0x00	External reset function of PB5 disabled
ATtiny12	0x0f	0x0f	CKSEL=1111 External Crystal / Ceramic Resonator
ATtiny12	0x0f	0x0e	CKSEL=1110 External Crystal / Ceramic Resonator
ATtiny12	0x0f	0x0d	CKSEL=1101 External Crystal / Ceramic Resonator
ATtiny12	0x0f	0x0c	CKSEL=1100 External Crystal / Ceramic Resonator
ATtiny12	0x0f	0x0b	CKSEL=1011 External Crystal / Ceramic Resonator
ATtiny12	0x0f	0x0a	CKSEL=1010 External Crystal / Ceramic Resonator
ATtiny12	0x0f	0x09	CKSEL=1001 External Low-Frequency Crystal
ATtiny12	0x0f	0x08	CKSEL=1000 External Low-Frequency Crystal
ATtiny12	0x0f	0x07	CKSEL=0111 External RC Ocsillator
ATtiny12	0x0f	0x06	CKSEL=0110 External RC Ocsillator
ATtiny12	0x0f	0x05	CKSEL=0101 External RC Ocsillator
ATtiny12	0x0f	0x04	CKSEL=0100 Internal RC Ocsillator
ATtiny12	0x0f	0x03	CKSEL=0011 Internal RC Ocsillator
ATtiny12	0x0f	0x02	CKSEL=0010 Internal RC Ocsillator ; default value
ATtiny12	0x0f	0x01	CKSEL=0001 External Clock
ATtiny12	0x0f	0x00	CKSEL=0000 External Clock
ATtiny13	0x80	0x00	Serial program downloading (SPI) enabled; [SPIEN=0]
ATtiny13	0x40	0x00	Preserve EEPROM memory through the Chip Erase cycle; [EESAVE=0]
ATtiny13	0x20	0x00	Watch-dog Timer always on; [WDTON=0]
ATtiny13	0x10	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATtiny13	0x0f	0x00	Ext. Clock; Start-up time: 14 CK + 0 ms; [CKSEL=00 SUT=00]
ATtiny13	0x0f	0x04	Ext. Clock; Start-up time: 14 CK + 4 ms; [CKSEL=00 SUT=01]
ATtiny13	0x0f	0x08	Ext. Clock; Start-up time: 14 CK + 64 ms; [CKSEL=00 SUT=10]
ATtiny13	0x0f	0x01	Int. RC Osc. 4.8 MHz; Start-up time: 14 CK + 0 ms; [CKSEL=01 SUT=00] 
ATtiny13	0x0f	0x05	Int. RC Osc. 4.8 MHz; Start-up time: 14 CK + 4 ms; [CKSEL=01 SUT=01] 
ATtiny13	0x0f	0x09	Int. RC Osc. 4.8 MHz; Start-up time: 14 CK + 64 ms; [CKSEL=01 SUT=10]
ATtiny13	0x0f	0x02	Int. RC Osc. 9.6 MHz; Start-up time: 14 CK + 0 ms; [CKSEL=10 SUT=00] 
ATtiny13	0x0f	0x06	Int. RC Osc. 9.6 MHz; Start-up time: 14 CK + 4 ms; [CKSEL=10 SUT=01] 
ATtiny13	0x0f	0x0a	Int. RC Osc. 9.6 MHz; Start-up time: 14 CK + 64 ms; [CKSEL=10 SUT=10]; default value
ATtiny13	0x0f	0x03	Int. RC Osc. 128 kHz; Start-up time: 14 CK + 0 ms; [CKSEL=11 SUT=00] 
ATtiny13	0x0f	0x07	Int. RC Osc. 128 kHz; Start-up time: 14 CK + 4 ms; [CKSEL=11 SUT=01] 
ATtiny13	0x0f	0x0b	Int. RC Osc. 128 kHz; Start-up time: 14 CK + 64 ms; [CKSEL=11 SUT=10]
ATtiny15	0x80	0x80	Brown-out detection level at VCC=2.7 V
ATtiny15	0x80	0x00	Brown-out detection level at VCC=4.0 V
ATtiny15	0x40	0x00	Brown-out detection enabled
ATtiny15	0x20	0x00	Serial program downloading (SPI) enabled
ATtiny15	0x10	0x00	External reset function of PB5 disabled
ATtiny15	0x03	0x03	CKSEL=11 Very quickly rising power
ATtiny15	0x03	0x02	CKSEL=10 Quickly rising power
ATtiny15	0x03	0x01	CKSEL=01 Slowly rising power
ATtiny15	0x03	0x00	CKSEL=00 Slowly rising power
ATtiny22	0x20	0x00	Serial program downloading (SPI) enabled
ATtiny22	0x01	0x00	Internal RC oscillator enabled
ATtiny22	0x01	0x01	External clock enabled
ATtiny2313	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATtiny2313	0x40	0x00	Clock output on PORTD2; [CKOUT=0]
ATtiny2313	0x3f	0x00	Ext. Clock; Start-up time: 14 CK + 0   ms; [CKSEL=0000 SUT=00]
ATtiny2313	0x3f	0x10	Ext. Clock; Start-up time: 14 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATtiny2313	0x3f	0x20	Ext. Clock; Start-up time: 14 CK + 65  ms; [CKSEL=0000 SUT=10]
ATtiny2313	0x3f	0x02	Int. RC Osc. 4 MHz; Start-up time: 14 CK + 0   ms; [CKSEL=0010 SUT=00]
ATtiny2313	0x3f	0x12	Int. RC Osc. 4 MHz; Start-up time: 14 CK + 4.1 ms; [CKSEL=0010 SUT=01]
ATtiny2313	0x3f	0x22	Int. RC Osc. 4 MHz; Start-up time: 14 CK + 65  ms; [CKSEL=0010 SUT=10]
ATtiny2313	0x3f	0x04	Int. RC Osc. 8 MHz; Start-up time: 14 CK + 0   ms; [CKSEL=0100 SUT=00]
ATtiny2313	0x3f	0x14	Int. RC Osc. 8 MHz; Start-up time: 14 CK + 4.1 ms; [CKSEL=0100 SUT=01]
ATtiny2313	0x3f	0x24	Int. RC Osc. 8 MHz; Start-up time: 14 CK + 65  ms; [CKSEL=0100 SUT=10]; default value
ATtiny2313	0x3f	0x06	Int. RC Osc. 128 kHz; Start-up time: 14 CK + 0 ms; [CKSEL=0110 SUT=00] 
ATtiny2313	0x3f	0x16	Int. RC Osc. 128 kHz; Start-up time: 14 CK + 4 ms; [CKSEL=0110 SUT=01] 
ATtiny2313	0x3f	0x26	Int. RC Osc. 128 kHz; Start-up time: 14 CK + 64 ms;[CKSEL=0110 SUT=10]
ATtiny2313	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 14 CK + 4.1 ms; [CKSEL=1000 SUT=00]
ATtiny2313	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 14 CK + 65 ms;  [CKSEL=1000 SUT=01]
ATtiny2313	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 14 CK + 0 ms;   [CKSEL=1000 SUT=10]
ATtiny2313	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 14 CK + 4.1 ms; [CKSEL=1000 SUT=11]
ATtiny2313	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 14 CK + 65 ms;  [CKSEL=1001 SUT=00]
ATtiny2313	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 14 CK + 0 ms;   [CKSEL=1001 SUT=01]
ATtiny2313	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 14 CK + 4.1 ms; [CKSEL=1001 SUT=10]
ATtiny2313	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time: 14 CK + 65 ms;  [CKSEL=1001 SUT=11]
ATtiny2313	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 14 CK + 4.1 ms; [CKSEL=1010 SUT=00]
ATtiny2313	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 14 CK + 65 ms;  [CKSEL=1010 SUT=01]
ATtiny2313	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 14 CK + 0 ms;   [CKSEL=1010 SUT=10]
ATtiny2313	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 14 CK + 4.1 ms; [CKSEL=1010 SUT=11]
ATtiny2313	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 14 CK + 65 ms;  [CKSEL=1011 SUT=00]
ATtiny2313	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 14 CK + 0 ms;   [CKSEL=1011 SUT=01]
ATtiny2313	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 14 CK + 4.1 ms; [CKSEL=1011 SUT=10]
ATtiny2313	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time: 14 CK + 65 ms;  [CKSEL=1011 SUT=11]
ATtiny2313	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 14 CK + 4.1 ms; [CKSEL=1100 SUT=00]
ATtiny2313	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 14 CK + 65 ms;  [CKSEL=1100 SUT=01]
ATtiny2313	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 14 CK + 0 ms;   [CKSEL=1100 SUT=10]
ATtiny2313	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 14 CK + 4.1 ms; [CKSEL=1100 SUT=11]
ATtiny2313	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 14 CK + 65 ms;  [CKSEL=1101 SUT=00]
ATtiny2313	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 14 CK + 0 ms;   [CKSEL=1101 SUT=01]
ATtiny2313	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 14 CK + 4.1 ms; [CKSEL=1101 SUT=10]
ATtiny2313	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time: 14 CK + 65 ms;  [CKSEL=1101 SUT=11]
ATtiny2313	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 14 CK + 4.1 ms; [CKSEL=1110 SUT=00]
ATtiny2313	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 14 CK + 65 ms;  [CKSEL=1110 SUT=01]
ATtiny2313	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 14 CK + 0 ms;   [CKSEL=1110 SUT=10]
ATtiny2313	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 14 CK + 4.1 ms; [CKSEL=1110 SUT=11]
ATtiny2313	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 14 CK + 65 ms;  [CKSEL=1111 SUT=00]
ATtiny2313	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 14 CK + 0 ms;   [CKSEL=1111 SUT=01]
ATtiny2313	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 14 CK + 4.1 ms; [CKSEL=1111 SUT=10]
ATtiny2313	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time: 14 CK + 65 ms;  [CKSEL=1111 SUT=11]
ATtiny24	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATtiny24	0x40	0x00	Clock output on PORTB2; [CKOUT=0]
ATtiny24	0x3f	0x00	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0000 SUT=00]
ATtiny24	0x3f	0x10	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATtiny24	0x3f	0x20	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0000 SUT=10]
ATtiny24	0x3f	0x02	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0010 SUT=00]
ATtiny24	0x3f	0x12	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0010 SUT=01]
ATtiny24	0x3f	0x22	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0010 SUT=10]; default value
ATtiny24	0x3f	0x04	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0100 SUT=00]
ATtiny24	0x3f	0x14	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0100 SUT=01]
ATtiny24	0x3f	0x24	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0100 SUT=10]
ATtiny24	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms; [CKSEL=0110 SUT=00] 
ATtiny24	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4 ms; [CKSEL=0110 SUT=01] 
ATtiny24	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32K CK/14 CK + 64 ms; [CKSEL=0110 SUT=10] 
ATtiny24	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1000 SUT=00]   
ATtiny24	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1000 SUT=01]   
ATtiny24	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1000 SUT=10]   
ATtiny24	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1000 SUT=11]   
ATtiny24	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1001 SUT=00]   
ATtiny24	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1001 SUT=01]   
ATtiny24	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1001 SUT=10]   
ATtiny24	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1001 SUT=11]   
ATtiny24	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1010 SUT=00]   
ATtiny24	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1010 SUT=01]   
ATtiny24	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1010 SUT=10]   
ATtiny24	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1010 SUT=11]   
ATtiny24	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1011 SUT=00]   
ATtiny24	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1011 SUT=01]   
ATtiny24	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1011 SUT=10]   
ATtiny24	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1011 SUT=11]   
ATtiny24	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1100 SUT=00]   
ATtiny24	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1100 SUT=01]   
ATtiny24	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1100 SUT=10]   
ATtiny24	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1100 SUT=11]   
ATtiny24	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1101 SUT=00]   
ATtiny24	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1101 SUT=01]   
ATtiny24	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1101 SUT=10]   
ATtiny24	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1101 SUT=11]   
ATtiny24	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1110 SUT=00]   
ATtiny24	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1110 SUT=01]   
ATtiny24	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1110 SUT=10]   
ATtiny24	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1110 SUT=11]   
ATtiny24	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1111 SUT=00]   
ATtiny24	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1111 SUT=01]   
ATtiny24	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1111 SUT=10]   
ATtiny24	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1111 SUT=11]   
ATtiny25	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATtiny25	0x40	0x00	Clock output on PORTB4; [CKOUT=0]
ATtiny25	0x3f	0x00	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0000 SUT=00]
ATtiny25	0x3f	0x10	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATtiny25	0x3f	0x20	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0000 SUT=10]
ATtiny25	0x3f	0x01	PLL Clock; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4 ms; [CKSEL=0001 SUT=00]
ATtiny25	0x3f	0x11	PLL Clock; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4 ms; [CKSEL=0001 SUT=01]
ATtiny25	0x3f	0x21	PLL Clock; Start-up time PWRDWN/RESET: 1K CK/14 CK + 64 ms; [CKSEL=0001 SUT=10]
ATtiny25	0x3f	0x31	PLL Clock; Start-up time PWRDWN/RESET: 16K CK/14 CK + 64 ms; [CKSEL=0001 SUT=11]
ATtiny25	0x3f	0x02	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0010 SUT=00]
ATtiny25	0x3f	0x12	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0010 SUT=01]
ATtiny25	0x3f	0x22	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0010 SUT=10]; default value
ATtiny25	0x3f	0x03	ATtiny15 Comp: Int. RC Osc. 6.4 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0011 SUT=00]
ATtiny25	0x3f	0x13	ATtiny15 Comp: Int. RC Osc. 6.4 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0011 SUT=01]
ATtiny25	0x3f	0x23	ATtiny15 Comp: Int. RC Osc. 6.4 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0011 SUT=10]
ATtiny25	0x3f	0x33	ATtiny15 Comp: Int. RC Osc. 6.4 MHz; Start-up time PWRDWN/RESET: 1 CK/14 CK + 0 ms; [CKSEL=0011 SUT=11]
ATtiny25	0x3f	0x04	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0100 SUT=00]
ATtiny25	0x3f	0x14	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0100 SUT=01]
ATtiny25	0x3f	0x24	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0100 SUT=10]
ATtiny25	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms; [CKSEL=0110 SUT=00] 
ATtiny25	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4 ms; [CKSEL=0110 SUT=01] 
ATtiny25	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32K CK/14 CK + 64 ms; [CKSEL=0110 SUT=10] 
ATtiny25	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1000 SUT=00]   
ATtiny25	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1000 SUT=01]   
ATtiny25	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1000 SUT=10]   
ATtiny25	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1000 SUT=11]   
ATtiny25	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1001 SUT=00]   
ATtiny25	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1001 SUT=01]   
ATtiny25	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1001 SUT=10]   
ATtiny25	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1001 SUT=11]   
ATtiny25	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1010 SUT=00]   
ATtiny25	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1010 SUT=01]   
ATtiny25	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1010 SUT=10]   
ATtiny25	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1010 SUT=11]   
ATtiny25	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1011 SUT=00]   
ATtiny25	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1011 SUT=01]   
ATtiny25	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1011 SUT=10]   
ATtiny25	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1011 SUT=11]   
ATtiny25	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1100 SUT=00]   
ATtiny25	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1100 SUT=01]   
ATtiny25	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1100 SUT=10]   
ATtiny25	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1100 SUT=11]   
ATtiny25	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1101 SUT=00]   
ATtiny25	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1101 SUT=01]   
ATtiny25	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1101 SUT=10]   
ATtiny25	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1101 SUT=11]   
ATtiny25	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1110 SUT=00]   
ATtiny25	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1110 SUT=01]   
ATtiny25	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1110 SUT=10]   
ATtiny25	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1110 SUT=11]   
ATtiny25	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1111 SUT=00]   
ATtiny25	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1111 SUT=01]   
ATtiny25	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1111 SUT=10]   
ATtiny25	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1111 SUT=11]   
ATtiny26	0x40	0x00	CKOPT fuse (operation dependent of CKSEL fuses); [CKOPT=0]
ATtiny26	0xbf	0x01	PLL Clock; Start-up time: 1K CK + 0 ms; [CKSEL=0001 SUT=00]
ATtiny26	0xbf	0x11	PLL Clock; Start-up time: 1K CK + 4 ms; [CKSEL=0001 SUT=01]
ATtiny26	0xbf	0x21	PLL Clock; Start-up time: 1K CK + 64 ms; [CKSEL=0001 SUT=10]
ATtiny26	0xbf	0x31	PLL Clock; Start-up time: 16K CK + 64 ms; [CKSEL=0001 SUT=11]
ATtiny26	0xbf	0x80	Ext. Clock; Start-up time: 6 CK + 0 ms; [CKSEL=0000 SUT=00]
ATtiny26	0xbf	0x90	Ext. Clock; Start-up time: 6 CK + 4 ms; [CKSEL=0000 SUT=01]
ATtiny26	0xbf	0xa0	Ext. Clock; Start-up time: 6 CK + 64 ms; [CKSEL=0000 SUT=10]
ATtiny26	0xbf	0x81	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0001 SUT=00]
ATtiny26	0xbf	0x91	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0001 SUT=01]
ATtiny26	0xbf	0xa1	Int. RC Osc. 1 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0001 SUT=10]; default value
ATtiny26	0xbf	0x82	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0010 SUT=00]
ATtiny26	0xbf	0x92	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0010 SUT=01]
ATtiny26	0xbf	0xa2	Int. RC Osc. 2 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0010 SUT=10]
ATtiny26	0xbf	0x83	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0011 SUT=00]
ATtiny26	0xbf	0x93	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0011 SUT=01]
ATtiny26	0xbf	0xa3	Int. RC Osc. 4 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0011 SUT=10]
ATtiny26	0xbf	0x84	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 0 ms; [CKSEL=0100 SUT=00]
ATtiny26	0xbf	0x94	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0100 SUT=01]
ATtiny26	0xbf	0xa4	Int. RC Osc. 8 MHz; Start-up time: 6 CK + 64 ms; [CKSEL=0100 SUT=10]
ATtiny26	0xbf	0x85	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0101 SUT=00]
ATtiny26	0xbf	0x95	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0101 SUT=01]
ATtiny26	0xbf	0xa5	Ext. RC Osc.         -  0.9 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0101 SUT=10]
ATtiny26	0xbf	0xb5	Ext. RC Osc.         -  0.9 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0101 SUT=11]
ATtiny26	0xbf	0x86	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0110 SUT=00]
ATtiny26	0xbf	0x96	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0110 SUT=01]
ATtiny26	0xbf	0xa6	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0110 SUT=10]
ATtiny26	0xbf	0xb6	Ext. RC Osc. 0.9 MHz -  3.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0110 SUT=11]
ATtiny26	0xbf	0x87	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=0111 SUT=00]
ATtiny26	0xbf	0x97	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=0111 SUT=01]
ATtiny26	0xbf	0xa7	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=0111 SUT=10]
ATtiny26	0xbf	0xb7	Ext. RC Osc. 3.0 MHz -  8.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=0111 SUT=11]
ATtiny26	0xbf	0x88	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 0 ms; [CKSEL=1000 SUT=00]
ATtiny26	0xbf	0x98	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 4 ms; [CKSEL=1000 SUT=01]
ATtiny26	0xbf	0xa8	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 18 CK + 64 ms; [CKSEL=1000 SUT=10]
ATtiny26	0xbf	0xb8	Ext. RC Osc. 8.0 MHz - 12.0 MHz; Start-up time: 6 CK + 4 ms; [CKSEL=1000 SUT=11]
ATtiny26	0xbf	0x89	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 4 ms; [CKSEL=1001 SUT=00]
ATtiny26	0xbf	0x99	Ext. Low-Freq. Crystal; Start-up time: 1K CK + 64 ms; [CKSEL=1001 SUT=01]
ATtiny26	0xbf	0xa9	Ext. Low-Freq. Crystal; Start-up time: 32K CK + 64 ms; [CKSEL=1001 SUT=10]
ATtiny26	0xbf	0x8a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1010 SUT=00]
ATtiny26	0xbf	0x9a	Ext. Crystal/Resonator Low Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1010 SUT=01]
ATtiny26	0xbf	0xaa	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1010 SUT=10]
ATtiny26	0xbf	0xba	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1010 SUT=11]
ATtiny26	0xbf	0x8b	Ext. Crystal/Resonator Low Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1011 SUT=00]
ATtiny26	0xbf	0x9b	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1011 SUT=01]
ATtiny26	0xbf	0xab	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1011 SUT=10]
ATtiny26	0xbf	0xbb	Ext. Crystal/Resonator Low Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1011 SUT=11]
ATtiny26	0xbf	0x8c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1100 SUT=00]
ATtiny26	0xbf	0x9c	Ext. Crystal/Resonator Medium Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1100 SUT=01]
ATtiny26	0xbf	0xac	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1100 SUT=10]
ATtiny26	0xbf	0xbc	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1100 SUT=11]
ATtiny26	0xbf	0x8d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1101 SUT=00]
ATtiny26	0xbf	0x9d	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1101 SUT=01]
ATtiny26	0xbf	0xad	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1101 SUT=10]
ATtiny26	0xbf	0xbd	Ext. Crystal/Resonator Medium Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1101 SUT=11]
ATtiny26	0xbf	0x8e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 4 ms; [CKSEL=1110 SUT=00]
ATtiny26	0xbf	0x9e	Ext. Crystal/Resonator High Freq.; Start-up time: 258 CK + 64 ms; [CKSEL=1110 SUT=01]
ATtiny26	0xbf	0xae	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 0 ms; [CKSEL=1110 SUT=10]
ATtiny26	0xbf	0xbe	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 4 ms; [CKSEL=1110 SUT=11]
ATtiny26	0xbf	0x8f	Ext. Crystal/Resonator High Freq.; Start-up time: 1K CK + 64 ms; [CKSEL=1111 SUT=00]
ATtiny26	0xbf	0x9f	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 0 ms; [CKSEL=1111 SUT=01]
ATtiny26	0xbf	0xaf	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 4 ms; [CKSEL=1111 SUT=10]
ATtiny26	0xbf	0xbf	Ext. Crystal/Resonator High Freq.; Start-up time: 16K CK + 64 ms; [CKSEL=1111 SUT=11]
ATtiny261	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATtiny261	0x40	0x00	Clock output on PORTB5; [CKOUT=0]
ATtiny261	0x3f	0x00	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0000 SUT=00]
ATtiny261	0x3f	0x10	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0000 SUT=01]
ATtiny261	0x3f	0x20	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms;  [CKSEL=0000 SUT=10]
ATtiny261	0x3f	0x01	PLL Clock; Start-up time PWRDWN/RESET: 1K CK/14 CK + 8 ms; [CKSEL=0001 SUT=00]
ATtiny261	0x3f	0x11	PLL Clock; Start-up time PWRDWN/RESET: 16K CK/14 CK + 8 ms; [CKSEL=0001 SUT=01]
ATtiny261	0x3f	0x21	PLL Clock; Start-up time PWRDWN/RESET: 1K CK/14 CK + 68 ms; [CKSEL=0001 SUT=10]
ATtiny261	0x3f	0x31	PLL Clock; Start-up time PWRDWN/RESET: 16K CK/14 CK + 68 ms; [CKSEL=0001 SUT=11]
ATtiny261	0x3f	0x02	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0010 SUT=00]
ATtiny261	0x3f	0x12	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0010 SUT=01]
ATtiny261	0x3f	0x22	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0010 SUT=10]; default value
ATtiny261	0x3f	0x03	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0011 SUT=00]
ATtiny261	0x3f	0x13	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0011 SUT=01]
ATtiny261	0x3f	0x23	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0011 SUT=10]
ATtiny261	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1 CK 4 ms; [CKSEL=0100 SUT=00]
ATtiny261	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1 CK + 64 ms; [CKSEL=0100 SUT=01]
ATtiny261	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32 CK + 64 ms; [CKSEL=0100 SUT=10]
ATtiny261	0x3f	0x08	Ext. Ceramic Res.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1000 SUT=00]   
ATtiny261	0x3f	0x18	Ext. Ceramic Res.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1000 SUT=01]   
ATtiny261	0x3f	0x28	Ext. Ceramic Res.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1000 SUT=10]   
ATtiny261	0x3f	0x38	Ext. Ceramic Res.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1000 SUT=11]   
ATtiny261	0x3f	0x09	Ext. Ceramic Res.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1001 SUT=00]   
ATtiny261	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1001 SUT=01]   
ATtiny261	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1001 SUT=10]   
ATtiny261	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1001 SUT=11]   
ATtiny261	0x3f	0x0a	Ext. Ceramic Res.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1010 SUT=00]   
ATtiny261	0x3f	0x1a	Ext. Ceramic Res.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1010 SUT=01]   
ATtiny261	0x3f	0x2a	Ext. Ceramic Res.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1010 SUT=10]   
ATtiny261	0x3f	0x3a	Ext. Ceramic Res.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1010 SUT=11]   
ATtiny261	0x3f	0x0b	Ext. Ceramic Res.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1011 SUT=00]   
ATtiny261	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1011 SUT=01]   
ATtiny261	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1011 SUT=10]   
ATtiny261	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1011 SUT=11]   
ATtiny261	0x3f	0x0c	Ext. Ceramic Res.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1100 SUT=00]   
ATtiny261	0x3f	0x1c	Ext. Ceramic Res.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1100 SUT=01]   
ATtiny261	0x3f	0x2c	Ext. Ceramic Res.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1100 SUT=10]   
ATtiny261	0x3f	0x3c	Ext. Ceramic Res.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1100 SUT=11]   
ATtiny261	0x3f	0x0d	Ext. Ceramic Res.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1101 SUT=00]   
ATtiny261	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1101 SUT=01]   
ATtiny261	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1101 SUT=10]   
ATtiny261	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1101 SUT=11]   
ATtiny261	0x3f	0x0e	Ext. Ceramic Res.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1110 SUT=00]   
ATtiny261	0x3f	0x1e	Ext. Ceramic Res.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1110 SUT=01]   
ATtiny261	0x3f	0x2e	Ext. Ceramic Res.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1110 SUT=10]   
ATtiny261	0x3f	0x3e	Ext. Ceramic Res.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1110 SUT=11]   
ATtiny261	0x3f	0x0f	Ext. Ceramic Res.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1111 SUT=00]   
ATtiny261	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1111 SUT=01]   
ATtiny261	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1111 SUT=10]   
ATtiny261	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1111 SUT=11]   
ATtiny44	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATtiny44	0x40	0x00	Clock output on PORTB2; [CKOUT=0]
ATtiny44	0x3f	0x00	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0000 SUT=00]
ATtiny44	0x3f	0x10	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATtiny44	0x3f	0x20	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0000 SUT=10]
ATtiny44	0x3f	0x02	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0010 SUT=00]
ATtiny44	0x3f	0x12	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0010 SUT=01]
ATtiny44	0x3f	0x22	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0010 SUT=10]; default value
ATtiny44	0x3f	0x04	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0100 SUT=00]
ATtiny44	0x3f	0x14	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0100 SUT=01]
ATtiny44	0x3f	0x24	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0100 SUT=10]
ATtiny44	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms; [CKSEL=0110 SUT=00] 
ATtiny44	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4 ms; [CKSEL=0110 SUT=01] 
ATtiny44	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32K CK/14 CK + 64 ms; [CKSEL=0110 SUT=10] 
ATtiny44	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1000 SUT=00]   
ATtiny44	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1000 SUT=01]   
ATtiny44	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1000 SUT=10]   
ATtiny44	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1000 SUT=11]   
ATtiny44	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1001 SUT=00]   
ATtiny44	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1001 SUT=01]   
ATtiny44	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1001 SUT=10]   
ATtiny44	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1001 SUT=11]   
ATtiny44	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1010 SUT=00]   
ATtiny44	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1010 SUT=01]   
ATtiny44	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1010 SUT=10]   
ATtiny44	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1010 SUT=11]   
ATtiny44	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1011 SUT=00]   
ATtiny44	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1011 SUT=01]   
ATtiny44	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1011 SUT=10]   
ATtiny44	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1011 SUT=11]   
ATtiny44	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1100 SUT=00]   
ATtiny44	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1100 SUT=01]   
ATtiny44	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1100 SUT=10]   
ATtiny44	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1100 SUT=11]   
ATtiny44	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1101 SUT=00]   
ATtiny44	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1101 SUT=01]   
ATtiny44	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1101 SUT=10]   
ATtiny44	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1101 SUT=11]   
ATtiny44	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1110 SUT=00]   
ATtiny44	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1110 SUT=01]   
ATtiny44	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1110 SUT=10]   
ATtiny44	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1110 SUT=11]   
ATtiny44	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1111 SUT=00]   
ATtiny44	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1111 SUT=01]   
ATtiny44	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1111 SUT=10]   
ATtiny44	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1111 SUT=11]   
ATtiny45	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATtiny45	0x40	0x00	Clock output on PORTB4; [CKOUT=0]
ATtiny45	0x3f	0x00	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0000 SUT=00]
ATtiny45	0x3f	0x10	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATtiny45	0x3f	0x20	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0000 SUT=10]
ATtiny45	0x3f	0x01	PLL Clock; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4 ms; [CKSEL=0001 SUT=00]
ATtiny45	0x3f	0x11	PLL Clock; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4 ms; [CKSEL=0001 SUT=01]
ATtiny45	0x3f	0x21	PLL Clock; Start-up time PWRDWN/RESET: 1K CK/14 CK + 64 ms; [CKSEL=0001 SUT=10]
ATtiny45	0x3f	0x31	PLL Clock; Start-up time PWRDWN/RESET: 16K CK/14 CK + 64 ms; [CKSEL=0001 SUT=11]
ATtiny45	0x3f	0x02	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0010 SUT=00]
ATtiny45	0x3f	0x12	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0010 SUT=01]
ATtiny45	0x3f	0x22	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0010 SUT=10]; default value
ATtiny45	0x3f	0x03	ATtiny15 Comp: Int. RC Osc. 6.4 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0011 SUT=00]
ATtiny45	0x3f	0x13	ATtiny15 Comp: Int. RC Osc. 6.4 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0011 SUT=01]
ATtiny45	0x3f	0x23	ATtiny15 Comp: Int. RC Osc. 6.4 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0011 SUT=10]
ATtiny45	0x3f	0x33	ATtiny15 Comp: Int. RC Osc. 6.4 MHz; Start-up time PWRDWN/RESET: 1 CK/14 CK + 0 ms; [CKSEL=0011 SUT=11]
ATtiny45	0x3f	0x04	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0100 SUT=00]
ATtiny45	0x3f	0x14	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0100 SUT=01]
ATtiny45	0x3f	0x24	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0100 SUT=10]
ATtiny45	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms; [CKSEL=0110 SUT=00] 
ATtiny45	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4 ms; [CKSEL=0110 SUT=01] 
ATtiny45	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32K CK/14 CK + 64 ms; [CKSEL=0110 SUT=10] 
ATtiny45	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1000 SUT=00]   
ATtiny45	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1000 SUT=01]   
ATtiny45	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1000 SUT=10]   
ATtiny45	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1000 SUT=11]   
ATtiny45	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1001 SUT=00]   
ATtiny45	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1001 SUT=01]   
ATtiny45	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1001 SUT=10]   
ATtiny45	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1001 SUT=11]   
ATtiny45	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1010 SUT=00]   
ATtiny45	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1010 SUT=01]   
ATtiny45	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1010 SUT=10]   
ATtiny45	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1010 SUT=11]   
ATtiny45	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1011 SUT=00]   
ATtiny45	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1011 SUT=01]   
ATtiny45	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1011 SUT=10]   
ATtiny45	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1011 SUT=11]   
ATtiny45	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1100 SUT=00]   
ATtiny45	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1100 SUT=01]   
ATtiny45	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1100 SUT=10]   
ATtiny45	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1100 SUT=11]   
ATtiny45	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1101 SUT=00]   
ATtiny45	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1101 SUT=01]   
ATtiny45	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1101 SUT=10]   
ATtiny45	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1101 SUT=11]   
ATtiny45	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1110 SUT=00]   
ATtiny45	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1110 SUT=01]   
ATtiny45	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1110 SUT=10]   
ATtiny45	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1110 SUT=11]   
ATtiny45	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1111 SUT=00]   
ATtiny45	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1111 SUT=01]   
ATtiny45	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1111 SUT=10]   
ATtiny45	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1111 SUT=11]   
ATtiny461	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATtiny461	0x40	0x00	Clock output on PORTB5; [CKOUT=0]
ATtiny461	0x3f	0x00	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0000 SUT=00]
ATtiny461	0x3f	0x10	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0000 SUT=01]
ATtiny461	0x3f	0x20	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms;  [CKSEL=0000 SUT=10]
ATtiny461	0x3f	0x01	PLL Clock; Start-up time PWRDWN/RESET: 1K CK/14 CK + 8 ms; [CKSEL=0001 SUT=00]
ATtiny461	0x3f	0x11	PLL Clock; Start-up time PWRDWN/RESET: 16K CK/14 CK + 8 ms; [CKSEL=0001 SUT=01]
ATtiny461	0x3f	0x21	PLL Clock; Start-up time PWRDWN/RESET: 1K CK/14 CK + 68 ms; [CKSEL=0001 SUT=10]
ATtiny461	0x3f	0x31	PLL Clock; Start-up time PWRDWN/RESET: 16K CK/14 CK + 68 ms; [CKSEL=0001 SUT=11]
ATtiny461	0x3f	0x02	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0010 SUT=00]
ATtiny461	0x3f	0x12	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0010 SUT=01]
ATtiny461	0x3f	0x22	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0010 SUT=10]; default value
ATtiny461	0x3f	0x03	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0011 SUT=00]
ATtiny461	0x3f	0x13	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0011 SUT=01]
ATtiny461	0x3f	0x23	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0011 SUT=10]
ATtiny461	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1 CK 4 ms; [CKSEL=0100 SUT=00]
ATtiny461	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1 CK + 64 ms; [CKSEL=0100 SUT=01]
ATtiny461	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32 CK + 64 ms; [CKSEL=0100 SUT=10]
ATtiny461	0x3f	0x08	Ext. Ceramic Res.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1000 SUT=00]   
ATtiny461	0x3f	0x18	Ext. Ceramic Res.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1000 SUT=01]   
ATtiny461	0x3f	0x28	Ext. Ceramic Res.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1000 SUT=10]   
ATtiny461	0x3f	0x38	Ext. Ceramic Res.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1000 SUT=11]   
ATtiny461	0x3f	0x09	Ext. Ceramic Res.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1001 SUT=00]   
ATtiny461	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1001 SUT=01]   
ATtiny461	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1001 SUT=10]   
ATtiny461	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1001 SUT=11]   
ATtiny461	0x3f	0x0a	Ext. Ceramic Res.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1010 SUT=00]   
ATtiny461	0x3f	0x1a	Ext. Ceramic Res.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1010 SUT=01]   
ATtiny461	0x3f	0x2a	Ext. Ceramic Res.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1010 SUT=10]   
ATtiny461	0x3f	0x3a	Ext. Ceramic Res.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1010 SUT=11]   
ATtiny461	0x3f	0x0b	Ext. Ceramic Res.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1011 SUT=00]   
ATtiny461	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1011 SUT=01]   
ATtiny461	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1011 SUT=10]   
ATtiny461	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1011 SUT=11]   
ATtiny461	0x3f	0x0c	Ext. Ceramic Res.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1100 SUT=00]   
ATtiny461	0x3f	0x1c	Ext. Ceramic Res.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1100 SUT=01]   
ATtiny461	0x3f	0x2c	Ext. Ceramic Res.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1100 SUT=10]   
ATtiny461	0x3f	0x3c	Ext. Ceramic Res.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1100 SUT=11]   
ATtiny461	0x3f	0x0d	Ext. Ceramic Res.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1101 SUT=00]   
ATtiny461	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1101 SUT=01]   
ATtiny461	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1101 SUT=10]   
ATtiny461	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1101 SUT=11]   
ATtiny461	0x3f	0x0e	Ext. Ceramic Res.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1110 SUT=00]   
ATtiny461	0x3f	0x1e	Ext. Ceramic Res.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1110 SUT=01]   
ATtiny461	0x3f	0x2e	Ext. Ceramic Res.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1110 SUT=10]   
ATtiny461	0x3f	0x3e	Ext. Ceramic Res.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1110 SUT=11]   
ATtiny461	0x3f	0x0f	Ext. Ceramic Res.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1111 SUT=00]   
ATtiny461	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1111 SUT=01]   
ATtiny461	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1111 SUT=10]   
ATtiny461	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1111 SUT=11]   
ATtiny84	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATtiny84	0x40	0x00	Clock output on PORTB2; [CKOUT=0]
ATtiny84	0x3f	0x00	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0000 SUT=00]
ATtiny84	0x3f	0x10	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATtiny84	0x3f	0x20	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0000 SUT=10]
ATtiny84	0x3f	0x02	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0010 SUT=00]
ATtiny84	0x3f	0x12	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0010 SUT=01]
ATtiny84	0x3f	0x22	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0010 SUT=10]; default value
ATtiny84	0x3f	0x04	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0100 SUT=00]
ATtiny84	0x3f	0x14	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0100 SUT=01]
ATtiny84	0x3f	0x24	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0100 SUT=10]
ATtiny84	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms; [CKSEL=0110 SUT=00] 
ATtiny84	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4 ms; [CKSEL=0110 SUT=01] 
ATtiny84	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32K CK/14 CK + 64 ms; [CKSEL=0110 SUT=10] 
ATtiny84	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1000 SUT=00]   
ATtiny84	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1000 SUT=01]   
ATtiny84	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1000 SUT=10]   
ATtiny84	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1000 SUT=11]   
ATtiny84	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1001 SUT=00]   
ATtiny84	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1001 SUT=01]   
ATtiny84	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1001 SUT=10]   
ATtiny84	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1001 SUT=11]   
ATtiny84	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1010 SUT=00]   
ATtiny84	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1010 SUT=01]   
ATtiny84	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1010 SUT=10]   
ATtiny84	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1010 SUT=11]   
ATtiny84	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1011 SUT=00]   
ATtiny84	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1011 SUT=01]   
ATtiny84	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1011 SUT=10]   
ATtiny84	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1011 SUT=11]   
ATtiny84	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1100 SUT=00]   
ATtiny84	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1100 SUT=01]   
ATtiny84	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1100 SUT=10]   
ATtiny84	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1100 SUT=11]   
ATtiny84	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1101 SUT=00]   
ATtiny84	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1101 SUT=01]   
ATtiny84	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1101 SUT=10]   
ATtiny84	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1101 SUT=11]   
ATtiny84	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1110 SUT=00]   
ATtiny84	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1110 SUT=01]   
ATtiny84	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1110 SUT=10]   
ATtiny84	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1110 SUT=11]   
ATtiny84	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1111 SUT=00]   
ATtiny84	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1111 SUT=01]   
ATtiny84	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1111 SUT=10]   
ATtiny84	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1111 SUT=11]   
ATtiny85	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATtiny85	0x40	0x00	Clock output on PORTB4; [CKOUT=0]
ATtiny85	0x3f	0x00	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0000 SUT=00]
ATtiny85	0x3f	0x10	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4.1 ms; [CKSEL=0000 SUT=01]
ATtiny85	0x3f	0x20	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 65 ms;  [CKSEL=0000 SUT=10]
ATtiny85	0x3f	0x01	PLL Clock; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4 ms; [CKSEL=0001 SUT=00]
ATtiny85	0x3f	0x11	PLL Clock; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4 ms; [CKSEL=0001 SUT=01]
ATtiny85	0x3f	0x21	PLL Clock; Start-up time PWRDWN/RESET: 1K CK/14 CK + 64 ms; [CKSEL=0001 SUT=10]
ATtiny85	0x3f	0x31	PLL Clock; Start-up time PWRDWN/RESET: 16K CK/14 CK + 64 ms; [CKSEL=0001 SUT=11]
ATtiny85	0x3f	0x02	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0010 SUT=00]
ATtiny85	0x3f	0x12	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0010 SUT=01]
ATtiny85	0x3f	0x22	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0010 SUT=10]; default value
ATtiny85	0x3f	0x03	ATtiny15 Comp: Int. RC Osc. 6.4 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0011 SUT=00]
ATtiny85	0x3f	0x13	ATtiny15 Comp: Int. RC Osc. 6.4 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0011 SUT=01]
ATtiny85	0x3f	0x23	ATtiny15 Comp: Int. RC Osc. 6.4 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0011 SUT=10]
ATtiny85	0x3f	0x33	ATtiny15 Comp: Int. RC Osc. 6.4 MHz; Start-up time PWRDWN/RESET: 1 CK/14 CK + 0 ms; [CKSEL=0011 SUT=11]
ATtiny85	0x3f	0x04	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0100 SUT=00]
ATtiny85	0x3f	0x14	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0100 SUT=01]
ATtiny85	0x3f	0x24	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0100 SUT=10]
ATtiny85	0x3f	0x06	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 0 ms; [CKSEL=0110 SUT=00] 
ATtiny85	0x3f	0x16	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1K CK/14 CK + 4 ms; [CKSEL=0110 SUT=01] 
ATtiny85	0x3f	0x26	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32K CK/14 CK + 64 ms; [CKSEL=0110 SUT=10] 
ATtiny85	0x3f	0x08	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1000 SUT=00]   
ATtiny85	0x3f	0x18	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1000 SUT=01]   
ATtiny85	0x3f	0x28	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1000 SUT=10]   
ATtiny85	0x3f	0x38	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1000 SUT=11]   
ATtiny85	0x3f	0x09	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1001 SUT=00]   
ATtiny85	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1001 SUT=01]   
ATtiny85	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1001 SUT=10]   
ATtiny85	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1001 SUT=11]   
ATtiny85	0x3f	0x0a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1010 SUT=00]   
ATtiny85	0x3f	0x1a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1010 SUT=01]   
ATtiny85	0x3f	0x2a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1010 SUT=10]   
ATtiny85	0x3f	0x3a	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1010 SUT=11]   
ATtiny85	0x3f	0x0b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1011 SUT=00]   
ATtiny85	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1011 SUT=01]   
ATtiny85	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1011 SUT=10]   
ATtiny85	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1011 SUT=11]   
ATtiny85	0x3f	0x0c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1100 SUT=00]   
ATtiny85	0x3f	0x1c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1100 SUT=01]   
ATtiny85	0x3f	0x2c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1100 SUT=10]   
ATtiny85	0x3f	0x3c	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1100 SUT=11]   
ATtiny85	0x3f	0x0d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1101 SUT=00]   
ATtiny85	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1101 SUT=01]   
ATtiny85	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1101 SUT=10]   
ATtiny85	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1101 SUT=11]   
ATtiny85	0x3f	0x0e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1110 SUT=00]   
ATtiny85	0x3f	0x1e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1110 SUT=01]   
ATtiny85	0x3f	0x2e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1110 SUT=10]   
ATtiny85	0x3f	0x3e	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1110 SUT=11]   
ATtiny85	0x3f	0x0f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1111 SUT=00]   
ATtiny85	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1111 SUT=01]   
ATtiny85	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1111 SUT=10]   
ATtiny85	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1111 SUT=11]   
ATtiny861	0x80	0x00	Divide clock by 8 internally; [CKDIV8=0]
ATtiny861	0x40	0x00	Clock output on PORTB5; [CKOUT=0]
ATtiny861	0x3f	0x00	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms;   [CKSEL=0000 SUT=00]
ATtiny861	0x3f	0x10	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0000 SUT=01]
ATtiny861	0x3f	0x20	Ext. Clock; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms;  [CKSEL=0000 SUT=10]
ATtiny861	0x3f	0x01	PLL Clock; Start-up time PWRDWN/RESET: 1K CK/14 CK + 8 ms; [CKSEL=0001 SUT=00]
ATtiny861	0x3f	0x11	PLL Clock; Start-up time PWRDWN/RESET: 16K CK/14 CK + 8 ms; [CKSEL=0001 SUT=01]
ATtiny861	0x3f	0x21	PLL Clock; Start-up time PWRDWN/RESET: 1K CK/14 CK + 68 ms; [CKSEL=0001 SUT=10]
ATtiny861	0x3f	0x31	PLL Clock; Start-up time PWRDWN/RESET: 16K CK/14 CK + 68 ms; [CKSEL=0001 SUT=11]
ATtiny861	0x3f	0x02	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0010 SUT=00]
ATtiny861	0x3f	0x12	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0010 SUT=01]
ATtiny861	0x3f	0x22	Int. RC Osc. 8 MHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0010 SUT=10]; default value
ATtiny861	0x3f	0x03	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 0 ms; [CKSEL=0011 SUT=00]
ATtiny861	0x3f	0x13	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 4 ms; [CKSEL=0011 SUT=01]
ATtiny861	0x3f	0x23	WD. Osc. 128 kHz; Start-up time PWRDWN/RESET: 6 CK/14 CK + 64 ms; [CKSEL=0011 SUT=10]
ATtiny861	0x3f	0x04	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1 CK 4 ms; [CKSEL=0100 SUT=00]
ATtiny861	0x3f	0x14	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 1 CK + 64 ms; [CKSEL=0100 SUT=01]
ATtiny861	0x3f	0x24	Ext. Low-Freq. Crystal; Start-up time PWRDWN/RESET: 32 CK + 64 ms; [CKSEL=0100 SUT=10]
ATtiny861	0x3f	0x08	Ext. Ceramic Res.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1000 SUT=00]   
ATtiny861	0x3f	0x18	Ext. Ceramic Res.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1000 SUT=01]   
ATtiny861	0x3f	0x28	Ext. Ceramic Res.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1000 SUT=10]   
ATtiny861	0x3f	0x38	Ext. Ceramic Res.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1000 SUT=11]   
ATtiny861	0x3f	0x09	Ext. Ceramic Res.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1001 SUT=00]   
ATtiny861	0x3f	0x19	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1001 SUT=01]   
ATtiny861	0x3f	0x29	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1001 SUT=10]   
ATtiny861	0x3f	0x39	Ext. Crystal Osc.; Frequency 0.4-0.9 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1001 SUT=11]   
ATtiny861	0x3f	0x0a	Ext. Ceramic Res.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1010 SUT=00]   
ATtiny861	0x3f	0x1a	Ext. Ceramic Res.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1010 SUT=01]   
ATtiny861	0x3f	0x2a	Ext. Ceramic Res.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1010 SUT=10]   
ATtiny861	0x3f	0x3a	Ext. Ceramic Res.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1010 SUT=11]   
ATtiny861	0x3f	0x0b	Ext. Ceramic Res.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1011 SUT=00]   
ATtiny861	0x3f	0x1b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1011 SUT=01]   
ATtiny861	0x3f	0x2b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1011 SUT=10]   
ATtiny861	0x3f	0x3b	Ext. Crystal Osc.; Frequency 0.9-3.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1011 SUT=11]   
ATtiny861	0x3f	0x0c	Ext. Ceramic Res.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1100 SUT=00]   
ATtiny861	0x3f	0x1c	Ext. Ceramic Res.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1100 SUT=01]   
ATtiny861	0x3f	0x2c	Ext. Ceramic Res.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1100 SUT=10]   
ATtiny861	0x3f	0x3c	Ext. Ceramic Res.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1100 SUT=11]   
ATtiny861	0x3f	0x0d	Ext. Ceramic Res.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1101 SUT=00]   
ATtiny861	0x3f	0x1d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1101 SUT=01]   
ATtiny861	0x3f	0x2d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1101 SUT=10]   
ATtiny861	0x3f	0x3d	Ext. Crystal Osc.; Frequency 3.0-8.0 MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1101 SUT=11]   
ATtiny861	0x3f	0x0e	Ext. Ceramic Res.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 4.1 ms; [CKSEL=1110 SUT=00]   
ATtiny861	0x3f	0x1e	Ext. Ceramic Res.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 258 CK/14 CK + 65 ms;  [CKSEL=1110 SUT=01]   
ATtiny861	0x3f	0x2e	Ext. Ceramic Res.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 0 ms;   [CKSEL=1110 SUT=10]   
ATtiny861	0x3f	0x3e	Ext. Ceramic Res.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 4.1 ms; [CKSEL=1110 SUT=11]   
ATtiny861	0x3f	0x0f	Ext. Ceramic Res.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 1K CK /14 CK + 65 ms;  [CKSEL=1111 SUT=00]   
ATtiny861	0x3f	0x1f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 0 ms;   [CKSEL=1111 SUT=01]   
ATtiny861	0x3f	0x2f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 4.1 ms; [CKSEL=1111 SUT=10]   
ATtiny861	0x3f	0x3f	Ext. Crystal Osc.; Frequency 8.0-    MHz; Start-up time PWRDWN/RESET: 16K CK/14 CK + 65 ms;  [CKSEL=1111 SUT=11]   
